Assessment Requirements for AURETR125 Test, charge and replace batteries and jump-start vehicles

Release: 1

Assessment Requirements for AURETR125 Test, charge and replace batteries and jump-start vehicles

Modification History

Release	Comments
Release 1	This version first released with AUR Automotive Retail, Service and Repair Training Package Version 6.0

Performance Evidence

The candidate must demonstrate the ability to complete the tasks outlined in the elements, performance criteria and foundation skills of this unit, including evidence of the ability to:

test two different types of automotive batteries

charge two batteries, in which the work must involve:

slow or trickle charging one battery

rapid charging the second battery

remove and replace batteries from two different vehicles or machinery

jump-start two different vehicles or machinery.

Knowledge Evidence

The candidate must be able to demonstrate knowledge to complete the tasks outlined in the elements, performance criteria and foundation skills of this unit, including knowledge of:

methods to locate and interpret information required to test, charge and replace batteries and jump-start vehicles, including:

battery and vehicle manufacturer specifications

safety data sheets (SDS)

workplace procedures required to test, charge and replace batteries and jump-start vehicles, including:

testing batteries

charging batteries

replacing batteries

jump-starting vehicles

establishing serviceability of tools and equipment

documentation procedures

housekeeping procedures, including:

examination of tools and equipment

storage of equipment

identification, tagging and isolation of faulty equipment

disposal of excess materials

recycling procedures

workplace health and safety (WHS) policies and procedures relating to testing, charging and replacing batteries and jump-start vehicles, including procedures for:

safely operating:

battery testing equipment

battery charging equipment

selecting and using personal protective equipment (PPE), including safety glasses

identifying hazards and controlling risks associated with:

battery, vehicle and machinery movement before carrying out work

wearing jewellery while working around high current wiring systems

identifying hybrid vehicles

identifying battery electric vehicles

environmental requirements relating to testing, charging and replacing batteries and jump-starting vehicles, including procedures for:

following safety data sheets (SDS) to trap, store and dispose of toxic and corrosive substances

disposing of or recycling batteries

tools and equipment required for testing, charging and replacing batteries and jump-starting vehicles, including:

load testing devices

hydrometers

multimeters

jumper leads

battery chargers

battery cleaning materials

difference between voltage and current

key features and uses of batteries, including:

lead acid batteries, including deep cycle batteries

gel batteries

absorbed glass mat batteries

calcium batteries

lithium ion and lithium ion phosphate batteries

battery connection methods for 6 volt, 12 volt, 24 volt and 48 volt, including:

series

parallel

series parallel

battery classification methods, including:

cold cranking amps (CCA)

reserve capacity (RC)

amp hour rating

battery testing procedures, including:

testing safety requirements

visual inspection procedures

voltage drop testing

hydrometer testing

high rate discharge testing

battery charging procedures, including:

charging safety requirements

slow, fast and trickle charging

battery memory retention

battery replacement procedures, including:

determining battery specifications to suit vehicle or machinery manufacturer specifications, including correct:

voltage

CCA and RC ratings

replacement safety requirements

terminal disconnection

battery selection

battery installation and terminal connection

securing battery in vehicle

system recalibration procedures

battery jump-start procedures, including:

vehicle and personnel safety requirements

battery terminal disconnection

jumper lead connection and disconnection.

Assessment Conditions

Competency is to be assessed in the workplace or a simulated environment that accurately reflects performance in a real workplace setting.

Assessment must include direct observation of tasks.

Where assessment of competency includes third-party evidence, individuals must provide evidence that links them to the batteries that they have tested, charged, replaced and jump-started, e.g. repair orders.

Assessors must verify performance evidence through questioning on skills and knowledge to ensure correct interpretation and application.

The following resources must be made available:

automotive repair workplace or simulated workplace

workplace instructions

manufacturer battery specifications

PPE for testing, charging, removing and replacing batteries and jump-starting vehicles and machinery, including safety glasses

two different types of serviceable batteries

two different vehicles or machinery requiring jump-starting

tools, equipment and materials appropriate for battery testing, charging and replacement, including:

load testing device

hydrometer

multimeter

jumper leads

battery charger

battery cleaning materials.

Assessors of this unit must satisfy the requirements for assessors in applicable vocational education and training legislation, frameworks and/or standards.

Links

Companion Volume Implementation Guide is found on VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1