Assessment Requirements for CPCCCA2003 Erect and dismantle formwork for footings and slabs on ground

Release: 1

Assessment Requirements for CPCCCA2003 Erect and dismantle formwork for footings and slabs on ground

Modification History

Release 1.

Supersedes and equivalent to CPCCCA2003A Erect and dismantle formwork for footings and slabs on ground.

The unit of competency was updated to the Standards for Training Packages 2012.

This version first released with CPC Construction, Plumbing and Services Training Package Version 4.0.

Performance Evidence

To demonstrate competency in this unit, a person must:

form up on ground a slab of at least nine square metres, incorporating an edge rebate and internal corner to specifications

form up a step to one foundation excavation to specified masonry units.

In doing this, the person must meet the performance criteria for this unit.

Knowledge Evidence

To be competent in this unit, a person must demonstrate knowledge of:

jurisdictional work health and safety (WHS) and environmental legislation and regulations relating to erecting and dismantling formwork for footings and slabs on ground, including:

job safety analyses (JSAs)

safe work method statements (SWMSs)

safety data sheets (SDSs)

safety manuals and instructions for plant, tools and equipment

signage and barricades

personal protective equipment (PPE)

environmental and work site safety plans

requirements of Australian Standards and the National Construction Code (NCC) relating to erecting and dismantling formwork for footings and slabs on ground

workplace requirements for undertaking all aspects of erecting and dismantling formwork for footings and slabs on ground, including interpreting work orders and reporting problems using general construction terminology applicable to work tasks

processes for interpreting project plans and specifications for erecting and dismantling formwork for footings and slabs on ground, including use of signage and barricades and calculation of material quantity and quality requirements

environmental requirements for erecting and dismantling formwork for footings and slabs on ground, including those relating to:

clean-up

noise and dust

vibration

waste management

types, characteristics, uses and limitations of plant, tools and equipment used for erecting and dismantling formwork for footings and slabs on ground

use of formwork materials, processes for setting out and measuring, requirements of application and for line, level and plumb in construction projects, formwork techniques and quality requirements, including termite barriers

processes for:

safe dismantling of formwork, including preparation of materials for re-use

materials and equipment storage and maintenance, and environmentally friendly waste management.

Assessment Conditions

Assessors must satisfy the requirements for assessors contained in the Standards for Registered Training Organisations.

Assessment of performance must be undertaken in the workplace or in a simulated workplace environment. Tasks are to be performed to the level of proficiency and within the time limits expected in a workplace.

Assessors are responsible for ensuring that the person demonstrating competency has access to:

work site and specifications to formup a slab on ground and formup a step to a foundation excavation

appropriate documents, formwork materials, tools, equipment and PPE currently used in industry

requirements of appropriate sections of legislation and regulations

relevant workplace policies and procedures.

Links

Companion volumes to this training package are available at the VETNet website - https://vetnet.education.gov.au/Pages/TrainingDocs.aspx?q=7e15fa6a-68b8-4097-b099-030a5569b1ad