Assessment Requirements for CPCCDE4006 Demolish stressed panel structure and pre-cast panel structure

Release: 1

Assessment Requirements for CPCCDE4006 Demolish stressed panel structure and pre-cast panel structure

Modification History

Release 1	This version first released with CPC Construction, Plumbing and Services Training Package Release 5.0. New unit.

Performance Evidence

To demonstrate competency in this unit the candidate must demolish one stressed panel structure and one pre-cast panel structure.

After identifying and controlling hazards, the candidate, working as a part of a team, must demolish one stressed panel structure of not less than four metres high, not less than three metres wide and not less than two tonnes in weight and one pre-cast panel structure of not less than four metres high, not less than three metres wide and not less than two tonnes in weight.

In doing this, the candidate must meet the performance criteria for this unit.

Knowledge Evidence

To be competent in this unit, a candidate must demonstrate knowledge of:

the compliance requirements of the relevant Australian Standards, Building Code of Australia (BCA), model codes of practice, environmental and work health and safety (WHS) legislation

basic theory related to cable stressing as a reinforcement technology

calibration procedures related to stressing techniques and equipment

construction and steelfixing tensioning terminology

factors affecting concrete bonding, curing and strength

grouting equipment and procedures

job safety analysis (JSA)

safe work method statements (SWMS)

safety data sheets (SDS)

materials storage and environmentally friendly waste management

plans, drawings and specifications

processes for the calculation of material requirements

quality requirements

requirements and processes for recording stressing operations

plans containing position of cables, height of chairs, cable specifications, number of strands per cable and the stressing loads

types of structural elements, including slabs, beams, columns and ground anchors

types of structures, including buildings, bridges, towers, tanks, silos, stayed structures, offshore platforms, and underground and submerged structures

safe de-tensioning procedures and techniques

workplace and equipment safety requirements

public protection:

demolition rated scaffolding.

Assessment Conditions

Assessors must meet the requirements for assessors contained in the Standards for Registered Training Organisations.

Assessment of performance must be undertaken in the workplace or in a simulated workplace environment.

Assessors are responsible for ensuring that the candidate demonstrating competency has access to:

demolition worksite/s specifications for demolishing stressed panel and pre-cast panel structures

appropriate documents, materials, tools, equipment and personal protective equipment (PPE) currently used in industry

requirements of workplace policies, procedures and demolition plans.

Links

Companion volumes to this training package are available at the VETNet website - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=7e15fa6a-68b8-4097-b099-030a5569b1ad