Assessment Requirements for CPCCSG3017 Erect and install signs

Release: 1

Assessment Requirements for CPCCSG3017 Erect and install signs

Modification History

Release 1.

This version first released with CPC Construction, Plumbing and Services Training Package Version 2.

Revised unit of competency. Replaces superseded non-equivalent CPCCSI2007A Apply fasteners and fixings.

Performance Evidence

A person who demonstrates competency in this unit must satisfy all of the elements, performance criteria and foundation skills of this unit, and must erect and install two signs as follows:

one sign must measure at least 1200 x 2400 mm, be constructed of aluminium no more than 5 mm thick, and be fixed using appropriate fixings and fastenings to one of the following surfaces:

acrylic

glass

masonry

metal

plasterboard

plastic

timber

one sign must measure at least 1200 x 2400 mm, be constructed of aluminium no more than 5 mm thick, and be positioned as a freestanding sign to two aluminium posts or poles measuring no less than 90 x 90 mm.

In doing the above work, the person must:

check and confirm the need for planning permissions to install the signs in specified location

check and confirm the site for services and assets below ground

assess the sign installation requirements relevant to the work site, identifying potential risks and hazards and demonstrating measures to mitigate potential work site risks and hazards

ensure the structural integrity of the supporting background, including taking steps to ensure reinforcement is arranged if required

follow safety procedures when erecting and installing above signs

identify and select methods for erecting and installing above signs, including selecting tools, fasteners and fixings giving consideration to the characteristics of the signs

prepare the work site for installation and install the signs according to job requirements.

Knowledge Evidence

A person demonstrating competency in this unit must demonstrate knowledge of:

purpose and application of the following when erecting and installing signs:

safety data sheets (SDS)

safe work method statements (SWMS)

effect of mechanical and chemical fixings and fastenings used to install signs on different surfaces

load bearing specifications for a range of fastener and fixing measurements and calculations relating to material quantities

relevant Australian and New Zealand standards in relation to the installation of signs, including:

AS/NZS 3832 Electrical installations – Cold-cathode illumination systems

AS 1319 Safety signs for the occupational environment

statutory and regulatory authority requirements, particularly those relating to:

removal of waste products

storage of chemicals and materials

types and uses of tools and equipment used for installing signs

processes and practices for working safely around power sources, services and assets.

Assessment Conditions

Suitable assessment of performance requires:

equipment:

a range of fasteners and fixings used for erecting and installing signs

a range of tools and equipment used for erecting and installing various types of signs:

chamois

drills

ladder

levelling tools

measuring tapes and rules

post hole digger

personal protective equipment suited to installing signs

touch-up paint

materials:

one freestanding sign and one sign fixed to a surface

signs to be 1200 x 2400 mm, constructed of aluminium

signs to be installed

ready-mix concrete

contingencies:

engineering risk assessment may be required to confirm structural integrity of supporting wall or structure

local authority planning permission may be required in certain settings and locations

specifications:

Australian and New Zealand standards in relation to the installation of signs, including:

AS/NZS 3832 Electrical installations – Cold-cathode illumination systems

AS 1319 Safety signs for the occupational environment

SDS

SWMS

physical conditions:

installation may be required in indoor and outdoor settings

relationship with client:

sufficient contact to check and confirm requirements

relationships with team members:

work may be undertaken alone or with others

timeframe:

according to job requirements.

Assessor requirements

As a minimum, assessors must satisfy the assessor requirements in the Standards for Registered Training Organisations (RTOs) current at the time of assessment.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=7e15fa6a-68b8-4097-b099-030a5569b1ad