CPPPMT3042A Install physical termite barriers

Release: 1

CPPPMT3042A Install physical termite barriers

Modification History

Revised unit

Unit updated and equivalent to PRMPM42A Install physical termite barriers

Unit Descriptor

This unit of competency specifies the outcomes required to install physical termite barriers, including barriers that combine physical and chemical characteristics. The unit requires the ability to assess techniques and methods of construction, as well as techniques required to prevent termites gaining concealed access to a completed construction. It requires a thorough understanding of client requirements, and the application of company information in order to perform the task. The selection of appropriate equipment, materials and methods is essential for performing the task safely and efficiently. These work functions would be carried out according to company guidelines and statutory requirements.

Application of the Unit

This unit of competency supports pest management technicians responsible for the application of physical termite barriers in both pre- and post-construction stages, in domestic, commercial and industrial buildings.

Licensing/Regulatory Information

This unit may be an essential requirement for a timber pest work licence. The full requirements for different licences may vary in different states and territories.

Pre-Requisites

Not applicable.

Employability Skills Information

This unit contains employability skills.

Elements and Performance Criteria Pre-Content

Elements describe the essential outcomes of a unit of competency.	Performance criteria describe the performance needed to demonstrate achievement of the element. Where bold italicised text is used, further information is detailed in the required skills and knowledge section and the range statement. Assessment of performance is to be consistent with the evidence guide.

Elements and Performance Criteria

1	Plan for construction process.	1.1	Installation requirements for termite barrier are identified from work order, drawings and supervisor’s instructions.
1.2	Work site plan is reviewed and installation specification is selected to prevent concealed termite access according to work order and legislative, occupational health and safety (OHS) and company requirements.
1.3	Client is advised of installation procedure according to work order and company requirements.
1.4	Quality assurance requirements are recognised and adhered to according to company requirements.
1.5	Materials are selected and located in readiness for installation according to manufacturer specifications and OHS and company requirements.
1.6	Equipment and tools consistent with installation requirements are selected, serviceability is checked, and faults are reported to appropriate persons according to manufacturer specifications and OHS and company requirements.

2	Access and assess site.	2.1	Work site is accessed according to client and company requirements.
2.2	Installation method is reviewed according to work order and company requirements, and issues are clarified with appropriate persons.
2.3	Previous trades work is checked for possible effect on proposed installation of termite barrier according to company requirements.
2.4	Work site is assessed for access and safety issues according to legislative, OHS and company requirements.

3	Prepare site for installation.	3.1	Hazards are identified and risks controlled at the work site according to company, legislative, OHS and public health and safety requirements.
3.2	Usage pattern of work site is determined to ensure safety of personnel and efficient use of equipment and tools.
3.3	Factors affecting completion of work order are identified and appropriate persons promptly advised.

4	Prepare equipment.	4.1	Suitable personal protective equipment (PPE) is selected and used according to manufacturer specifications and legislative, OHS and company requirements.
4.2	Equipment and tools are selected and operational effectiveness is checked according to manufacturer specifications and legislative, OHS and company requirements.
4.3	Equipment and tools are set up according to manufacturer specifications and legislative, OHS and company requirements.
4.4	Equipment and tools are adjusted according to manufacturer specifications to suit operator’s requirements.

5	Install physical barrier.	5.1	Termite barrier is installed to concealed termite access points according to work order, manufacturer specifications and company requirements.
5.2	Installation of termite barrier is checked according to company requirements.
5.3	Work is conducted using safe operating practices according to manufacturer specifications and environmental, legislative, OHS and company requirements.

6	Restore work site and complete documentation.	6.1	Equipment, tools and waste are collected and removed according to work order, manufacturer specifications and legislative, OHS, company and environmental requirements.
6.2	Work site is restored according to work order, client requests and company requirements.
6.3	Equipment, tools and PPE are cleaned according to manufacturer specifications and environmental, OHS and company requirements.
6.4	Equipment, tools and PPE are safety checked and required maintenance is recorded according to manufacturer specifications and OHS and company requirements.
6.5	Cleaned equipment, tools and PPE are stored according to company requirements.
6.6	Collected waste is disposed of according to work order, manufacturer specifications and environmental, legislative, OHS and company requirements.
6.7	Client records are updated and regulatory and company documentation is completed and distributed according to legislative and company requirements.

Required Skills and Knowledge

This section describes the skills and knowledge required for this unit.
Required skills
skills to work safely when: identifying hazards and controlling risks manual handling customer service skills to: establish rapport with clients gain clients’ trust perceive and respond to clients’ attitudes to pest problems language, literacy and numeracy skills for: communicating clearly and concisely verbally and in writing performing mathematical calculations required to measure length, area and volume reading and interpreting directions and safety instructions, including: equipment manuals material safety data sheets (MSDS) labels requesting advice or further information seeking and receiving feedback sourcing, organising and recording information planning and organising work, including: accurately estimating timeframes attending to detail in observing work site conditions scheduling efficiently self-management skills to work alone and in a team
Required knowledge
legislation, regulations, codes of practice and industry advisory standards that apply to the installation of physical termite barriers, including: OHS legislation relevant Australian standards relevant licence requirements company management structure and procedures, including: emergency response procedures manual-handling techniques OHS procedures reporting channels construction methods and materials, such as: concrete slabs footings wall frame materials hazardous substances in the workplace installation equipment product knowledge, including manufacturer specifications for equipment and products being used subterranean termite ecology as related to termite barrier installation work order specifications

Evidence Guide

The evidence guide provides advice on assessment and must be read in conjunction with the performance criteria, required skills and knowledge, range statement and the Assessment Guidelines for the Training Package.
Overview of assessment	This unit of competency could be assessed by observing practical demonstration in the field and by reviewing the outcome of at least two complete termite barrier installations under normal industry operating conditions, or if this is not practicable, in a simulated work environment.
Critical aspects for assessment and evidence required to demonstrate competency in this unit	A person who demonstrates competency in this unit must be able to provide evidence of the required skills and knowledge specified in this unit. In particular the person should demonstrate the ability to: carry out correct procedures prior to and during installation of physical termite barrier communicate to support team and ensure safe and effective workplace operations comply with: company policies and procedures, including quality assurance legislative and regulatory requirements product installation specifications identify hazards and risks associated with the installation safely and effectively use hand and power tools, plant and equipment achieve outcomes in relation to work order.
Context of and specific resources for assessment	Assessment of essential underpinning knowledge may be conducted in an off-site context. It is to comply with relevant regulatory or Australian standards’ requirements. Resource implications for assessment include access to: suitable work site or venue suitable equipment and materials PPE equipment operating manuals and MSDS company procedures and manufacturer specifications and MSDS plain English version of relevant statutes and procedures relevant databases and information assessment instruments, including personal planner and assessment record book.
Method of assessment	Assessment methods must: satisfy the endorsed Assessment Guidelines of the Property Services Training Package include direct observation of tasks in real or simulated work conditions, with questioning to confirm the ability to consistently identify and correctly interpret the essential underpinning knowledge required for practical application reinforce the integration of employability skills with workplace tasks and job roles confirm that competency is verified and able to be transferred to other circumstances and environments.
Guidance information for assessment	Reasonable adjustments for people with disabilities must be made to assessment processes where required. This could include access to modified equipment and other physical resources, and the provision of appropriate assessment support. Assessment processes and techniques should as far as is practical take into account the language, literacy and numeracy capacity of the candidate in relation to the competency being assessed. This unit could be assessed on its own or in combination with other units relevant to the job function, for example: CPPPMT3002A Assess pest management options CPPPMT3005A Modify environment to manage pests CPPPMT3007A Implement pest management plans CPPPMT3043A Prepare and present pest management proposals.

Range Statement

The range statement relates to the unit of competency as a whole. It allows for different work environments and situations that may affect performance. Bold italicised wording, if used in the performance criteria, is detailed below. Essential operating conditions that may be present with training and assessment (depending on the work situation, needs of the candidate, accessibility of the item, and local industry and regional contexts) may also be included.
Installation may include:	identifiable areas that require protection method of combining specifications and work order requirements procedures from company training and reference manuals specifications from company manuals techniques conveyed during training courses.
Work order information may include:	access to work site, including: timing of access access and egress points budget allocations completion times and dates dress and presentation requirements job requirements and tasks legislative and local government requirements OHS requirements and emergency response procedures requirements for working in isolated and remote locations resource requirements – equipment and materials specific client requirements of technician, such as: noise control relationships with other customer activities sensitivity of occupants to pests or pest management use of signage and barriers work schedules work site contact persons.
Legislative requirements may include:	Australian standards, quality assurance and certification requirements award and enterprise agreements industry advisory standards and codes, such as: building codes dangerous goods codes relevant commonwealth, state and territory legislation and local government regulations that affect company operation, such as: anti-discrimination and diversity chemical controls consumer protection legislation environmental protection issues equal employment opportunity freedom of information industrial relations installers’ licence requirements motor and commercial vehicle transportation motor licence and endorsement regulations OHS Acts and regulations privacy public health trade practices workplace consultative arrangements.
Occupational health and safety (also known as workplace health and safety) requirements may relate to:	allergic reactions, such as contact dermatitis communication devices for remote and isolated locations, such as: mobile phone two-way radio emergency procedures for contact with toxic substances, such as: splashes in eye or on skin inhalation ingestion hazard identification and risk assessment mechanisms hierarchy of hazard control procedures industry advisory standards information provided by national registration authority and state government authorities, such as: agriculture environment protection health primary industry injury and dangerous occurrence reporting national and industry codes of practice OHS control procedures, such as: health and safety plans job plans job safety analyses risk assessments safe operating practices and procedures safe work instructions safe work method statements safety, induction and refresher training selection and use of PPE and clothing appropriate to hazard up-to-date electrical test and tag compliance use of chemicals according to MSDS use of epoxies or other bonding agents according to MSDS use of residual current devices use, storage and maintenance of equipment according to manufacturer specifications and equipment operating manuals.
Company requirements may include:	access and equity policy, principles and practice business and performance plans client communication procedures client confidentiality procedures client service standards company goals, objectives, plans, systems and processes company issued identification badge, card or pass company policies and procedures defined resource parameters dress and presentation requirements duty of care, code of conduct and code of ethics emergency response and evacuation procedures employer and employee rights and responsibilities establishing operator identity with client internal communication channels and reporting procedures maintenance procedures for equipment and PPE OHS policies and procedures personnel practices and guidelines policies and procedures relating to own role, responsibility and delegation quality and continuous improvement processes and standards records and information systems and processes training (induction and refresher) materials work site access security clearance procedures.
Clients may include:	architects bodies corporate builders building supervisors companies or organisations developers maintenance managers owners persons in control of work processes property agents or managers tenants.
Materials may include:	adhesives termite barrier components.
Manufacturer specifications may include:	emergency response resources equipment operating manuals government publications instructional guides MSDS other resources supplied by manufacturer, such as: laminated cards notices wall posters product labels safety instructions pre-printed on equipment.
Equipment and tools may include:	adhesive applicators angle grinders bolsters brushes and brooms drills: power rechargeable generators hammers hoses knives measuring tapes or rules power leads rollers safety switch equipment screwdrivers sheet metal or utility cutters or snips shovels.
Appropriate persons may include:	clients colleagues managers persons in control of work site supervisors.
Work sites may include:	buildings commercial construction areas domestic construction areas industrial construction areas vacant land prepared for construction.
Previous trades work may include:	blocklaying bricklaying carpentry concreting electrical plumbing.
Termite barrier may include:	bonding materials that adhere proprietary products to substrate proprietary products that provide a barrier at termite access point(s) proprietary products used in combination that provide a comprehensive barrier in line with regulatory requirements visual barriers formed as a result of construction techniques, such as exposed concrete slab edges.
Hazards may include:	allergic reactions to chemicals, pests or equipment, including latex allergies blood and blood-stained products confined or restricted spaces contaminated clothing, materials and equipment damaged or inappropriate equipment dust and fibres electrical hazards arising from: cables electrical fittings: switches lights untested electrical equipment fatigue fire gas heights inadequate lighting and ventilation mobile or vehicle hazards around plant and vehicles moving and unguarded parts noise occupational violence and bullying poor personal hygiene practices release of substances with negative environmental impact spills, splashes and sprays unsafe manual-handling techniques, including awkward and repetitive postures unsafe underfoot conditions, such as slippery, uneven and rough surfaces work environment temperature extremes work in unfamiliar isolated or remote environments.
Public health and safety may affect:	animals clients’ staff company staff customers distributors facility users general public, including neighbours and bystanders inspectors retailers suppliers trade and service providers.
Personnel may include:	clients’ staff colleagues site visitors, including bystanders venue, facility, building or shopping centre staff and management.
Personal protective equipment may include:	communication equipment drinking fluids dust masks eye protection, such as: eyewashes and showers safety glasses face shields first aid kits appropriate to tasks and locations gloves hair nets hard hats long pants noise protection overalls, coveralls or other protective clothing safety shoes or boots safety harnesses soap and towels sunscreen washable sun hats.
Termite access points may include:	concrete shrinkage joints around slab penetrations construction joints perimeter cavities piers and sub-floor walls in suspended floor construction retainer walls.
Waste may be solid or liquid and include:	contaminated or hazardous biological waste used containers used or contaminated PPE.
Environmental requirements may include:	clean up, containment or isolation company policies and guidelines hazardous materials handling regulations, by-laws and guidelines of environmental protection agencies and government departments, such as: agriculture emergency services national parks and wildlife.
Client records may be a computer or manual file and include:	contact details customer files and databases details of previous: installations quotations government orders specific details about: site termite barrier installation.
Regulatory and company documentation may include:	accident and incident reports certificates and notices customer files and databases invoices and receipts job sheets logbooks OHS control procedures and forms risk assessments work diaries.

Unit Sector(s)

Pest management

Custom Content Section

Not applicable.