FPIHAR4202B Coordinate log recovery (hook tender)

Release: 1

FPIHAR4202B Coordinate log recovery (hook tender)

Modification History

Not Applicable

Unit Descriptor

Unit descriptor	This unit describes the outcomes required to coordinate operational planning and setting up of cable recovery systems, including supervision and coordination of rigging slingers, yarders, choker setters and chasers Compliance with licensing, legislative, regulatory or certification requirements may be required in various jurisdictions. This unit replaces FPIHAR4202A Coordinate log recovery (hook tender)

Application of the Unit

Application of the unit	The unit involves coordinating log recovery (hook tender) in a forest or farm forest setting The skills and knowledge required for competent workplace performance are to be used within the scope of the person's job and authority

Licensing/Regulatory Information

Refer to Unit Descriptor

Pre-Requisites

Prerequisite units

Employability Skills Information

Employability skills	This unit contains employability skills

Elements and Performance Criteria Pre-Content

Elements describe the essential outcomes of a unit of competency.	Performance criteria describe the performance needed to demonstrate achievement of the element. Where bold italicised text is used, further information is detailed in the required skills and knowledge section and the range statement. Assessment of performance is to be consistent with the evidence guide.

Elements and Performance Criteria

ELEMENT	PERFORMANCE CRITERIA
1. Prepare for hook tender operations	1.1. Applicable Occupational Health and Safety (OHS), environmental, legislative and organisational requirements relevant to coordinating log recovery (hook tender) are identified and followed 1.2. Work order is reviewed and checked with appropriate personnel 1.3. Type and quantity of cable recovery equipment are identified and assessed for safe working conditions and environmental protection measures 1.4. Equipment is selected appropriate to work requirements and checked for operational effectiveness in line with manufacturer's recommendations 1.5. Hooker and cable operations activities are planned in line with site procedures 1.6. Communication with others is established and maintained in line with OHS requirements
2. Plan cable system layout	2.1. Information essential to the planning of the cable system layout is obtained, evaluated and the site inspected for factors affecting harvesting operations and potential hazards 2.2. Landing location and size, hauling boundaries, access routes and construction requirements are provided to construction personnel 2.3. Cable system type is selected to provide optimum extraction rate for trees to be felled, considering site topography and codes of practice and minimising system design additions 2.4. General requirements for anchor points, backline and intermediate supports are identified and instructions given to fallers
3. Coordinate yarder and cable system set up	3.1. Rope sizes are selected for lines in line with the code of practice, yarder capacity and system design 3.2. Components and rigging are selected to meet code of practice requirements and system design 3.3. Components and lines are inspected during installation and set up 3.4. Site personnel are directed and assisted to layout lines, select anchors and position mobile backstops 3.5. Felled trees and extraction sequence are assessed for size, location and obstructions with recovery planned to minimise line shifts, log and environmental damage 3.6. Support trees are selected and directions provided for rigging 3.7. Unloaded and loaded system performance is checked and loads calculated to ensure they are within system and equipment capacity 3.8. Operations are monitored and procedural or system design changes to improve safety and payload efficiency noted and communicated
4. Coordinate rigging of spars, towers and trees	4.1. Cable system is checked from plans and operational requirements interpreted for tower, spars and support trees 4.2. Spars or support trees to be rigged, necessary guylines and required anchor points are checked from the plan or selected within guidelines provided, with trees topped in line with the code of practice 4.3. Rigging suitable for operational requirements, loads and rope sizes is selected to meet the code of practice and industry standards 4.4. Directions are provided to check components for wear, failure or missing parts prior to rigging, faults are identified and corrective action is taken 4.5. Rigging is coordinated on machine towers to prepare, assemble and fit operational lines in line with system design, prior to raising 4.6. Climbing and pass line equipment is identified to be operated in line with the code of practice 4.7. Guys positioning and rigging within location angle requirements of the code of practice to provide minimal difference in length and tension is coordinated 4.8. System components are checked to ensure they meet the code of practice for size, safe working load, layout, position, safety straps, joins, lead angles and operating angles
5. Coordinate line shifts and rigging modifications	5.1. Line shifts are anticipated and required rigging is prepared in advance 5.2. Limitations of system positioning or design are diagnosed and modifications planned in line with the code of practice 5.3. Operations are monitored and procedural changes to improve safety and payload efficiency noted and communicated 5.4. New support trees, anchor points and mobile tail anchor position are located and riggers assigned to prepare and rig these in line with system requirements 5.5. Breakout processes and equipment faults are recorded and reported to the appropriate personnel

Required Skills and Knowledge

REQUIRED SKILLS AND KNOWLEDGE
This describes the essential skills and knowledge and their level required for this unit
Required skills
Technical skills sufficient to use and maintain relevant tools, machinery and equipment; efficiently and safely coordinate hook tender operations Communication skills and interpersonal techniques sufficient to interact appropriately with colleagues and others in the workplace Literacy skills sufficient to accurately record and report workplace information, and maintain documentation Numeracy skills sufficient to estimate measure and calculate time required to complete a task Problem solving skills sufficient to identify problems and equipment faults and demonstrate appropriate response procedures
Required knowledge
Applicable Commonwealth, State or Territory legislation, regulations, standards, codes of practice and established safe practices relevant to the full range of processes for coordinating log recovery (hook tender) Environmental protection requirements, including the safe disposal of waste material and the cleaning of plant, tools and equipment Organisational and site standards, requirements, policies and procedures for coordinating log recovery (hook tender) Cable recovery operations and planning Rigging techniques Industry standard lengths Rigging and yarding operations Timber extraction methods Established communication channels and protocols Problem identification and resolution strategies and common fault finding techniques Types of tools and equipment and procedures for their use, operation and maintenance Appropriate mathematical procedures for estimating and measuring, including calculating time to complete tasks Procedures for recording and reporting workplace records and information

Evidence Guide

EVIDENCE GUIDE
The evidence guide provides advice on assessment and must be read in conjunction with the performance criteria, required skills and knowledge, range statement and the Assessment Guidelines for the Training Package.
Overview of assessment	A person who demonstrates competency in this unit must be able to provide evidence that they safely and efficiently coordinate hook tender operations within organisational requirements
Critical aspects for assessment and evidence required to demonstrate competency in this unit	The evidence required to demonstrate competency in this unit must be relevant to, and satisfy, all of the requirements of the elements of this unit and include demonstration of: following applicable Commonwealth, State or Territory legislative and regulatory requirements and codes of practice relevant to coordinating log recovery (hook tender) following organisational policies and procedures relevant to coordinating log recovery (hook tender) coordinating hook tender operations in line with the work order and within prescribed organisational tolerances planning the layout of cable systems in line with site conditions modifying rigging and coordinating line shifts in line with the hook tender's instructions
Context of and specific resources for assessment	Competency is to be assessed in the workplace or realistically simulated workplace Assessment is to occur under standard and authorised work practices, safety requirements and environmental constraints Assessment of required knowledge, other than confirmatory questions, will usually be conducted in an off-site context Assessment is to follow relevant regulatory or Australian Standards requirements The following resources should be made available: workplace location or simulated workplace materials and equipment relevant to undertaking work applicable to this unit specifications and work instructions
Method of assessment	Assessment must satisfy the endorsed Assessment Guidelines of the FPI11 Training Package Assessment methods must confirm consistency and accuracy of performance (over time and in a range of workplace relevant contexts) together with application of required knowledge Assessment must be by direct observation of tasks, with questioning on required knowledge and it must also reinforce the integration of employability skills Assessment methods must confirm the ability to access and correctly interpret and apply the required knowledge Assessment may be applied under project-related conditions (real or simulated) and require evidence of process Assessment must confirm a reasonable inference that competency is able not only to be satisfied under the particular circumstance, but is able to be transferred to other circumstances Assessment may be in conjunction with assessment of other units of competency The assessment environment should not disadvantage the candidate Assessment practices should take into account any relevant language or cultural issues related to Aboriginality, gender or language backgrounds other than English Where the participant has a disability, reasonable adjustment may be applied during assessment Language and literacy demands of the assessment task should not be higher than those of the work role

Range Statement

RANGE STATEMENT
The range statement relates to the unit of competency as a whole. It allows for different work environments and situations that may affect performance. Bold italicised wording, if used in the performance criteria, is detailed below. Essential operating conditions that may be present with training and assessment (depending on the work situation, needs of the candidate, accessibility of the item, and local industry and regional contexts) may also be included.
OHS requirements:	are to be in with applicable Commonwealth, State or Territory legislation and regulations, and organisational safety policies and procedures, and may include: personal protective equipment and clothing safety equipment first aid equipment fire fighting equipment hazard and risk control fatigue management elimination of hazardous materials and substances safe forest practices including required actions relating to forest fire manual handling including shifting, lifting and carrying
Environmental requirements may include:	legislation organisational policies and procedures workplace practices
Legislative requirements:	are to be in line with applicable Commonwealth, State or Territory legislation, regulations, certification requirements and codes of practice and may include: award and enterprise agreements industrial relations Australian Standards confidentiality and privacy OHS the environment equal opportunity anti-discrimination relevant industry codes of practice duty of care
Organisational requirements may include:	legal organisational and site guidelines policies and procedures relating to own role and responsibility quality assurance procedural manuals quality and continuous improvement processes and standards OHS, emergency and evacuation procedures ethical standards recording and reporting requirements equipment use and maintenance and storage requirements environmental management requirements (waste disposal, recycling and re-use guidelines)
Work order is to include:	instructions for coordinating hook tender operations from the work site and may include type size length quantity grade instructions for the environmental monitoring of work and procedures environmental care requirements relevant to the work
Appropriate personnel may include:	supervisors suppliers clients colleagues managers
Cable recovery equipment may include:	yarders spars rigging equipment cables
Environmental protection measures may include:	ground growth canopy general forest lean wind speed and direction fallen trees density of trees ground slope soil and water protection ground hazards obstacles contingencies for modifying operations during wet or other adverse weather conditions
Equipment is to include:	refer to cable recovery equipment procedures for equipment lock-out such as protecting operators and co-workers from accidental injury by isolating the machine
Hooker (hook tender)	is the cable logging team leader who decides which method of logging will be the fastest and most efficient, and also designs, plans and coordinates the establishment of cable recovery systems (the higher the hooker can get the logs off the ground means fewer broken logs, hang ups and snags)
Cable operations may include:	activities covering a full range of species, log sizes, falling and retention densities, slope, other environmental conditions the use of cable systems including high lead (no skyline), standing skyline and a running skyline with hauling both uphill and downhill logs attached optimising payload without exceeding the lift or haul capacity of the system
Communication may include:	verbal and non-verbal language constructive feedback active listening questioning to clarify and confirm understanding use of positive, confident and cooperative language use of language and concepts appropriate to individual social and cultural differences control of tone of voice body language
Landing	is the location where the yarder is positioned to receive the logs
Hauling boundaries	are designated forest coupes owned privately, by Government or by the forestry organisation with boundaries which fall within survey pegs for the land allocated for logging
Topography	is a map of the designated area showing terrain levels
System design additions are to include:	multispans blind leads bridling other techniques potentially reducing extraction efficiency
Yarder	is the crane-like vehicle which winches the timber from the felling site to the landing using a cable system
Lines are to include:	mainlines haulback lines skylines strawlines extensions guylines
Components may include:	carriages jacks butt rigging chokers grapples blocks sheaves ropes shackles pins tail rope straps intermediate supports
Anchors are to include:	anchors tailholds block stumps mobile backstops
Extraction sequence	is the method of removing the log from the work site with mechanical equipment and cables, considering site conditions and specific log location, in a way which minimises downtime and risk of snags, breakage and hang ups
Obstructions may include:	standing trees stumps rocks ground projections
Line shifts	are the moving of rigging lines from one area of operation to a new area
Support trees	are trees (with heads removed) which can act as spars and be rigged accordingly
Spars	are out-posted erections which provide elevation for the cables some distance from the yarder tower
Towers	are the crane like raised towers which the cables operate from to provide height for extraction of logs.
Guylines	support the tower or spar and other rigged erections to provide stability and strength during operation
Climbing and pass line equipment	are lines linked to the drum line for the purposes of climbing trees and spars
Guys	refer to guylines
Records and reports may include:	cable recovery operations extraction methods hazards incidents equipment malfunctions and may be: manual using a computer-based system or another appropriate organisational communication system

Unit Sector(s)

Unit sector	No sector assigned

Co-requisite units

Co-requisite units

Competency field

Competency field	Harvesting and Haulage