Assessment Requirements for ICPCBF221 Set up and produce basic guillotined product

Release: 1

Assessment Requirements for ICPCBF221 Set up and produce basic guillotined product

Modification History

Release	Comments
Release 1	This version first released with ICP Printing and Graphic Arts Training Package Version 1.0.

Performance Evidence

Evidence of the ability to:

demonstrate all safety devices on the machine

correctly set up (not including knife change) and produce TWO basic guillotined products (if possible, one large sheet and one small sheet) according to manufacturer’s and job specifications and enterprise procedures.

Note: If a specific volume or frequency is not stated, then evidence must be provided at least once.

Knowledge Evidence

To complete the unit requirements safely and effectively, the individual must:

identify health and safety factors for:

setting up and operating the machine

checking and adjusting the machine

maintaining the production process

handling knife blades during the knife change operation

shutting down or cleaning the machine

identify information concerning cutting that should be found in the job documentation or production control system

identify factors that:

indicate a new blade is needed

indicate the need to replace a cutting stick

should be considered when setting up a guillotine for cutting

indicate the need for machine lubrication

identify the difference between a sharp knife from a dull knife, and problems arising from continuously using a dull blade

explain how correct clamping pressure is determined for a given job

identify reporting procedures for when the machine malfunctions

explain treatment/disposal of guillotine waste

identify the part of the guillotine that should be checked if, after a cut:

top sheets are out-of-square

top sheets are creasing across the cut line

identify where information is found regarding correct types and methods of lubrication

list special operations that are essential when shutting down the machine

identify quality aspects to consider in a completed cutting job and when checking against the sample

list steps to take if the cutting result does not coincide with the sample

identify machine manuals, safety and other documentation relevant to this task, where they are kept, and the information included in them.

Assessment Conditions

Gather evidence to demonstrate consistent performance in conditions that are safe and replicate the workplace. Noise levels, production flow, interruptions and time variances must be typical of those experienced in the converting, binding and finishing field of work and include access to and use of facilities, equipment and materials used to set up and produce a basic guillotined product.

Assessors must satisfy NVR/AQTF assessor requirements.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.education.gov.au/Pages/TrainingDocs.aspx?q=a74b7a0f-a253-47e3-8be0-5d426e24131d