Assessment Requirements for ICPPRN262 Produce foil stamped product

Release: 1

Assessment Requirements for ICPPRN262 Produce foil stamped product

Modification History

Release	Comments
Release 1	This version first released with ICP Printing and Graphic Arts Training Package Version 1.0.

Performance Evidence

Evidence of the ability to:

operate a gold blocking or hot foil stamping machine ensuring an efficient production flow that maintains product quality standards. Any production problems are anticipated and rectified with minimum downtime. The machine is correctly shut down and cleaned according to work health and safety (WHS) guidelines

demonstrate use of control, monitoring and data entry systems

demonstrate an ability to find and use information relevant to the task from a variety of information sources

produce TWO foil stamped products (if possible including at least one in-line process if relevant) according to job specifications and enterprise procedures.

Note: If a specific volume or frequency is not stated, then evidence must be provided at least once.

Knowledge Evidence

To complete the unit requirements safely and effectively, the individual must:

Maintaining in-feed and delivery of reel or sheet or 3D object transportation section

identify WHS concerns when operating a transportation system

For reel systems only

explain why tracking the web is important to position and register

identify implications if web is not spliced correctly

list identification used for web splices

describe precautions to ensure rewound product is of consistent, acceptable quality

For sheet systems only

explain why sheets are fanned before loading into the press

describe impact printing double sheets has on the foil stamped product

list components which, if sheeted, can be adjusted to ensure correct delivery

explain how printed material below acceptable standard is identified

describe aspects of loading and ejection that need to be monitored

Maintaining the foil stamping process

identify major WHS concerns when foil stamping

describe considerations that contribute to determining the ideal press speed

explain at what interval the product should be checked for consistency

identify the cause of non-image areas of the print filling in

describe remedial action if the edges of the print are jagged

explain why the use of anti-set off spray is not recommended when foil stamping

describe how to adjust the machine to correct a shift in image position on the object

Shutdown and cleaning of the press

identify dangers of solvents and solutions used to clean the press and printing dyes

describe how dyes should be stored following printing

list the effect of poorly stored dyes

identify parts of the machine to be thoroughly cleaned following the print run

list components to be inspected for wear following the print run

identify records important for following or repeat prints

Information sources

locate machine manuals, safety and other documentation relevant to this task and outline information included.

Assessment Conditions

Gather evidence to demonstrate consistent performance in conditions that are safe and replicate the workplace. Noise levels, production flow, interruptions and time variances must be typical of those experienced in the printing field of work and include access to special purpose tools, equipment and materials.

Assessors must satisfy NVR/AQTF assessor requirements.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=a74b7a0f-a253-47e3-8be0-5d426e24131d