Assessment Requirements for MSFGG3030 Process glass by automatic machines

Release: 1

Assessment Requirements for MSFGG3030 Process glass by automatic machines

Modification History

Release 1. Supersedes and is equivalent to MSFGG3006 Process glass by automatic machines.

Performance Evidence

There must be evidence the candidate has completed the tasks outlined in the elements and performance criteria of this unit, and:

used automatic glass processing equipment for all of the following:

cutting from optimisation data

drilling

edging.

Knowledge Evidence

There must be evidence the candidate has knowledge of:

purpose and key provisions of Australian Standard AS/NZS 4667:2000 Quality requirements for cut-to-size and processed glass

workplace safety system requirements related to glass processing by automatic machine

work flow requirements in relation to glass processing

mathematical procedures for machine programming

qualities and characteristics of different types of glass, including hazards and handling requirements

features of software used in automatic processing in relation to design and file transfer

types, characteristics, safe use, maintenance and capabilities of computer-navigated and Computer Numerical Control (CNC) machines:

bevellers and brilliant cutter

diamond saws

edgers

laser glass cutters

straight line and shape annealed and laminated glass cutters

water jet machines

marking tools

measuring tools, including tape measures, L-squares and straight edges

templates

types of information that needs to be entered into automatic machines:

glass thickness

size

type

stock sheet size

off-cut sizes

procedures for automatic machine processing, the types of problems that may occur and how to avoid and respond

quality indicators for processed glass

procedures for the recording, reporting and maintenance of workplace records and information.

Assessment Conditions

Skills must have been demonstrated in the workplace or in a simulated environment that reflects workplace conditions and contingencies. The following conditions must be met for this unit:

use of suitable facilities, equipment and resources, including:

equipment, tools and materials to complete tasks in the Performance Evidence

glass product to be processed

work orders

workplace procedures.

Assessors must satisfy the NVR/AQTF mandatory competency requirements for assessors.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=0601ab95-583a-4e93-b2d4-cfb27b03ed73