MSMRV318 Fit cladding to a recreational vehicle

Release: 1

MSMRV318 Fit cladding to a recreational vehicle

Modification History

Release 1 - New unit.

Application

This unit of competency covers the skills and knowledge required to fit side cladding and roof skin to a recreational vehicle. The work will be carried out in a recreational vehicle manufacturing facility.

This unit of competency covers the preparation for, fitting of, and clean-up after the fitting of cladding and roof skin.

The operator will be required to work to procedures, and follow plans/specifications for what is required.

This unit of competency applies to an individual working alone or as part of a team/work group and working in liaison with other shift team members.

No licensing, legislative or certification requirements apply to this unit at the time of publication.

Pre-requisite Unit

Nil

Competency Field

Operations

Unit Sector

Elements and Performance Criteria

Elements describe the essential outcomes	Performance criteria describe the performance needed to demonstrate achievement of the element
1	Plan the work	1.1	Review the requirements of the work
1.2	Check required tools and jigs are available at the worksite
1.3	Check required materials and components are available at the worksite
1.4	Identify any hazards and the related hazard controls
1.5	Check the hazard controls are in place and operational
1.6	Query any items that are different to usual and clarify requirements

2	Fit the side frame cladding in accordance with procedures	2.1	Use relevant hazard controls, including personal protective equipment (PPE)
2.2	Place the cladding in the required position
2.3	Clamp/hold cladding in place as required
2.4	Drill holes/make any penetrations required
2.5	Fix cladding to frame as required
2.6	Trim cladding as required
2.7	Complete fitting of side frame cladding as required

3	Fit the roof skin in accordance with procedures	3.1	Use relevant hazard controls, including PPE
3.2	Place the skin in the required position
3.3	Clamp/hold skin in place as required
3.4	Drill holes/make any penetrations required
3.5	Fix skin to frame as required
3.6	Trim skin as required
3.7	Complete fitting of roof skin as required

4	Finish fitting the cladding and roof skin	4.1	Check cladding and roof skin has been fitted correctly and make any required adjustments
4.2	Clean up recreational vehicle and work area, leaving it ready for the next job
4.3	Segregate and handle waste in accordance with procedures
4.4	Complete any required documentation/records

Foundation Skills

This section describes those language, literacy, numeracy and employment skills that are essential to performance.

Foundation skills essential to performance are explicit in the performance criteria of this unit of competency.

Range of Conditions

This field allows for different work environments and conditions that may affect performance. Essential operating conditions that may be present (depending on the work situation, needs of the candidate, accessibility of the item, and local industry and regional contexts) are included.
Regulatory framework	The latest version of all legislation, regulations, industry codes of practice and Australian/international standards, or the version specified by the local regulatory authority, must be used, and include one or more of the following: legislative requirements, including work health and safety (WHS) industry codes of practice and guidelines environmental regulations and guidelines Australian and other standards licence and certification requirements
Procedures	All operations must be performed in accordance with relevant procedures. Procedures are written, verbal, visual, computer-based or in some other form, and include one or more of the following: work instructions standard operating procedures (SOPs) safe work method statements (SWMS) temporary instructions any similar instructions provided for the smooth running of the plant
Hazards	Hazards include one or more of the following: heat, dust or other atmospheric hazards electricity gas equipment failures industrial (machinery, equipment and product) noise, rotational equipment or vibration hazardous products and materials unauthorised personnel sharp edges, protrusions or obstructions slippery surfaces, spills or leaks other hazards that might arise
Routine problems	Routine problems must be resolved by applying known solutions. Routine problems are predictable and include one or more of the following: equipment/plant/machine malfunction variations in process conditions variations in materials or contamination of materials equipment, tool, die or mould damage product faults tooling problems Known solutions are drawn from one or more of the following: procedures training remembered experience Non-routine problems must be reported according to relevant procedures.

Unit Mapping Information

No equivalent unit

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=d1287d36-dff4-4e9f-ad2c-9d6270054027