Assessment Requirements for AUMGTG001 Install fixed and moveable glass components on vehicles

Release: 2

AUMGTG001 Install fixed and moveable glass components on vehicles

Modification History

Release	Comment
Release 1	Unit updated to reflect the new standards for Training Packages Replaces AUMGTG3001 Install fixed and moveable glass components
Release 2	Updated for clarity and policy adherence

Performance Evidence

Before competency can be determined, individuals must have competently installed glass components on vehicles on a minimum of two occasions.

Individuals must demonstrate they can:

interpret job information

mark out and fabricate templates for glass components

select appropriate glass sealants, adhesives, tools and equipment

prepare, install and adjust fixed and moveable glass components according to workplace procedures and work health and safety (WHS) requirements, including:

vehicle protection measures

personal protective equipment – safety glasses, gloves and coveralls

leak test installed glass components

check, clean and maintain tools and equipment, and store appropriately

clean and recycle appropriate material

complete workplace documentation relating to installation.

Knowledge Evidence

The candidate must be able to demonstrate knowledge to complete the tasks outlined in the elements and performance criteria of this unit. This includes:

workplace procedures and WHS requirements relating to installing fixed and moveable glass components on vehicles

workplace quality guidelines for installing glass components in vehicles

work documentation covering procedures, specifications, schedules and work plans

template measuring and marking out procedures

cutting procedures for vehicle panels and trim

installation procedures for fixed, bonded and moveable glass components

urethane, rubber and butyl installation methods

bonded glass installation methods.

Assessment Conditions

Assessors must satisfy SNR/AQTF assessor requirements.

Competency is to be assessed in the workplace or a simulated environment that accurately reflects performance in a real workplace setting.

Where assessment of competency includes third-party evidence, individuals must provide evidence that links them to the vehicles on which they have worked, e.g. work sheets.

Assessors must verify performance evidence through questioning on skills and knowledge to ensure correct interpretation and application.

The following resources must be made available:

automotive manufacturing workplace or simulated workplace

tools and equipment required for installing glass components

automotive vehicle or simulated frame for glass installation

materials to produce templates for glass components

fixed and movable glass components

work orders and job specifications

WHS requirements for installing glass components on vehicles, including:

vehicle protection equipment

personal protective equipment, including safety glasses, gloves and coveralls

workplace procedures to install fixed and moveable glass components on vehicles

workplace documentation relating to installing glass components on vehicles, including:

customer details

glass warranty information

work sheets.

Links

Companion Volume Implementation Guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=bd587669-08b3-4cd5-85f0-f9fa0c6304c1