Assessment Requirements for AURKTD101 Diagnose and repair mobile plant suspension systems

Release: 1

Assessment Requirements for AURKTD101 Diagnose and repair mobile plant suspension systems

Modification History

Release	Comments
Release 1	This version first released with AUR Automotive Retail, Service and Repair Training Package Version 6.0

Performance Evidence

The candidate must demonstrate the ability to complete the tasks outlined in the elements, performance criteria and foundation skills of this unit, including evidence of the ability to:

diagnose and repair a fault in at least three mobile plant suspension systems as follows:

at least one gas charged hydraulic suspension

at least two of the following:

pivoting axle suspension

solid rubber suspension

hydraulic suspension.

Knowledge Evidence

The candidate must be able to demonstrate knowledge to complete the tasks outlined in the elements, performance criteria and foundation skills of this unit, including knowledge of:

methods to locate and interpret information required to diagnose and repair mobile plant suspension systems, including:

information provided by customers and supervisors

manufacturer specifications and procedures or equivalent documentation

workplace procedures required to diagnose and repair mobile plant suspension systems, including:

establishing serviceability of tools and equipment

documentation procedures

housekeeping procedures, including:

examination of tools and equipment

storage of equipment

identification, tagging and isolation of faulty equipment

disposal of excess materials

recycling procedures

workplace health and safety (WHS) requirements relating to diagnosing and repairing mobile plant suspension systems, including procedures for:

suspension lock-out

isolating and stabilising machines

working with stored fluid pressures from accumulators

working with high pressure fluid hazards

using lifting, jacking and supporting equipment

environmental requirements relating to diagnosing and repairing mobile plant suspension systems

purpose and operation of mobile plant suspension systems and components, including:

suspension hydraulic circuitry

pivoting axle suspension

solid rubber suspension

gas charged hydraulic suspension

hydraulic suspension

pneumatic tyres

diagnostic testing procedures for mobile plant suspension systems, including procedures for analysing:

component wear

abnormal system noise

suspension cylinder

erratic operation

repair procedures for mobile plant suspension systems, including procedures for:

repairing and adjusting suspension components

recharging suspension cylinders

post-repair testing procedures for mobile plant suspension systems.

Assessment Conditions

Competency is to be assessed in the workplace or a simulated environment that accurately reflects performance in a real workplace setting.

Assessment must include direct observation of tasks.

Where assessment of competency includes third-party evidence, individuals must provide evidence that links them to the mobile plant suspension systems that they have worked on, e.g. repair orders.

Assessors must verify performance evidence through questioning on skills and knowledge to ensure correct interpretation and application.

The following resources must be made available:

automotive repair workplace or simulated workplace

workplace instructions

manufacturer mobile plant suspension system specifications

three different mobile plant suspension systems specified in the performance evidence with system faults

diagnostic equipment for mobile plant suspension systems

tools, equipment and materials appropriate for repairing and adjusting mobile plant suspension systems.

Assessors of this unit must satisfy the requirements for assessors in applicable vocational education and training legislation, frameworks and/or standards.

Links

Companion Volume Implementation Guide is found on VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1