Assessment Requirements for AURKTJ012 Remove, inspect and fit earthmoving and off-the-road wheel and rim assemblies

Release: 1

Assessment Requirements for AURKTJ012 Remove, inspect and fit earthmoving and off-the-road wheel and rim assemblies

Modification History

Release	Comment
Release 1	New unit of competency.

Performance Evidence

The candidate must demonstrate they can perform the following according to the standards defined in the elements, performance criteria and foundation skills of this unit.

The candidate must demonstrate removing, inspecting, and refitting industrial earthmoving and off-the-road (OTR) wheel and rim assemblies that safely follows workplace procedures to meet required outcomes on a minimum of three occasions. The candidate must:

locate and interpret required documentation, policies and procedures

apply appropriate control measures to mitigate hazardous conditions in work environment and hazardous tyre, wheel and rim assembly conditions

use raising and supporting equipment to raise vehicle in accordance with workplace procedures

deflate tyre safely and in accordance with workplace procedures

remove wheel and rim assembly in accordance with workplace procedures

inflate tyre safely and in accordance with workplace procedures

monitor tyre, wheel and rim assembly throughout inflation of tyre

fit tyre, wheel and rim assembly including using the correct:

isolation procedures

tightening sequence

torque settings

inflation process and pressure

alignment

check and confirm the following prior to fastening:

component compatibility

tyre, wheel and rim component serviceability

correct assembly of wheel and rim assembly

safely lower vehicle

undertake post-work inspection and complete work processes, including storage of tools and equipment

transport and store tyre, wheel and rim assembly

complete workplace documentation, including:

relevant risk assessments

tyre, wheel and rim assembly change documentation.

The above work must be performed on tyres fitted to wheel assemblies and rim assemblies of not less than 600 mm (24 inches) nominal diameter. In the course of the work above, the candidate must:

utilise tyre handing equipment at least once.

prepare, clean and inspect tyre, wheel and rim assembly for damage and serviceability, recommending repair and replacement actions for each of the following wheel or rim configurations:

three piece wheel or rim assembly

five piece wheel or rim assembly

split wheel or rim assembly

Knowledge Evidence

The candidate must demonstrate the following knowledge:

Key policies and procedures for removing, inspecting and fitting earthmoving and OTR wheel and rim assemblies, including:

how to locate and interpret manufacturers specifications, applicable standards and workplace procedures for removing, inspecting and fitting earthmoving and off-the-road wheel and rim assemblies

applicable standards for removing, inspecting and fitting earthmoving and OTR wheel and rim assemblies

WHS requirements relevant to removing, inspecting and fitting earthmoving and OTR tyres

procedures relating to earthmoving and OTR wheel and rim assemblies:

fitting

hazard identification and risk control methods, including but not limited to those relating to:

hydraulic tooling

pneumatic tooling

torque measurement when tightening wheel or rim fasteners

inflation and deflation of tyres

inspection

pre-removal inspection

post-fitting inspection

raising, supporting and lowering procedures for mining and construction vehicles that include soft ground support procedures and systems

removal procedures of earthmoving and OTR wheel and rim assemblies:

methods for undoing wheel or rim fasteners

handling methods

two piece industrial rim

disk or demountable multi piece rim

one piece wheel and rim

Earthmoving and OTR vehicle tyres, wheels and rim assembly information including:

types and classifications of earthmoving and OTR tyres, wheels and rim assemblies

types of mounting systems for earthmoving and OTR wheel and rim assemblies.

Assessment Conditions

The assessment must:

include access to:

a workplace or simulated workplace that reflects workplace conditions - where simulation is used, it must reflect real working conditions by modelling industry operating conditions and contingencies, as well as, using suitable facilities, equipment and resources

repair orders and workplace instructions relating to removing, inspecting and fitting earthmoving and OTR wheel and rim assemblies

WHS requirements and workplace procedures relevant to removing, inspecting and fitting earthmoving and OTR wheel and rim assemblies

manufacturer specifications and procedures or equivalent documentation to remove, inspect and fit earthmoving and OTR wheel and rim assemblies

applicable standards relevant to removing, inspecting and fitting earthmoving and OTR wheel and rim assemblies

tyre handing equipment, including one of the following:

crane

earthmoving and OTR tyre handler

forklift

grab truck

integrated tool handler

earthmoving and OTR wheel and rim assemblies

WHS requirements relevant to removing, inspecting and fitting earthmoving and OTR wheel and rim assemblies

tools and equipment appropriate for removing and fitting earthmoving and OTR wheel and rim assemblies

tyre, wheel and rim assembly specifications and workplace instructions

operational vehicles with earthmoving and OTR wheel and rim assemblies

personal protective clothing and equipment required for the activities described in the performance evidence

be demonstrated in the workplace or in a simulated environment that reflects workplace conditions

be conducted in a safe environment

be assessed in compliance with relevant policies, procedures, processes and operational manuals directly related to the industry sector for which it is being assessed

confirm consistent performance can be applied in a range of relevant workplace circumstances.

Assessor requirements

Assessors of this unit must:

satisfy the assessor requirements in applicable vocational education and training legislation, frameworks and/or standards.

Links

Companion Volume Implementation Guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1