Assessment Requirements for AURLTE003 Analyse and evaluate faults in light vehicle engine and fuel systems

Release: 1

Assessment Requirements for AURLTE003 Analyse and evaluate faults in light vehicle engine and fuel systems

Modification History

Release	Comment
Release 1	New unit of competency.

Performance Evidence

Before competency can be determined, individuals must demonstrate they can perform the following according to the standards defined in this unit’s elements, performance criteria, range of conditions and foundation skills:

analyse and evaluate a fault in the:

engine system of a light vehicle

fuel system of a different light vehicle

engine or fuel system of a third light vehicle.

Knowledge Evidence

Individuals must be able to demonstrate knowledge of:

work health and safety (WHS) and occupational health and safety (OHS) requirements relating to analysing and evaluating faults in light vehicle engine and fuel systems, including procedures for working with:

hot engine components and rotating engine components

hazardous substances, including:

diesel fuel

petrol fuel

engine oil and coolants

environmental requirements, including procedures for trapping, storing and disposing of fluids released from engine and fuel systems

principles and processes involved in planning and implementing analysis and evaluation of light vehicle engine and fuel system faults

design and planning of diagnostic procedures of light vehicle engine and fuel system faults, including procedures for diagnosing:

hydraulic faults

mechanical faults

electrical faults

procedures for analysing and evaluating light vehicle engine and fuel system faults, including:

system failure analysis

component failure analysis

types, functions, operation and limitations of the following engine and fuel systems:

petrol engines

diesel engines

petrol fuel systems

diesel fuel systems

testing procedures for light vehicle engine and fuel systems, including:

engine performance under load

fuel flow and pressure

cooling system performance under load

oil pressure

exhaust flow

types, functions, operation and limitations of diagnostic testing equipment required to analyse and evaluate faults in light vehicle engine and fuel systems

procedures for documenting and reporting the analysis and evaluation process

requirements of Australian Design Rules (ADRs) relating to light vehicle engine and fuel systems.

Assessment Conditions

Assessors must satisfy NVR/AQTF assessor requirements.

Competency is to be assessed in the workplace or a simulated environment that accurately reflects performance in a real workplace setting.

Assessment must include direct observation of tasks.

Where assessment of competency includes third-party evidence, individuals must provide evidence that links them to the light vehicle engine and fuel systems that they have worked on, e.g. repair orders.

Assessors must verify performance evidence through questioning on skills and knowledge to ensure correct interpretation and application.

The following resources must be made available:

automotive repair workplace or simulated workplace

workplace instructions

manufacturer light vehicle engine and fuel system specifications

three different light vehicles with engine and fuel system faults

diagnostic equipment for light vehicle engine and fuel systems

tools, equipment and materials appropriate for analysing and evaluating light vehicle engine and fuel systems.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1