AURPTA008 Service and repair post hole digging systems

Release: 1

AURPTA008 Service and repair post hole digging systems

Modification History

Release	Comment
Release 1	New unit of competency.

Application

This unit describes the performance outcomes required to service and repair faults in the post hole digging systems of outdoor power equipment according to manufacturer specifications. It involves preparing for the task, determining the service and repair requirements, carrying out the service and repair, performing post-repair testing, and completing workplace processes and documentation.

It applies to those working in the outdoor power equipment service and repair industry. The post hole digging systems may be powered by electric or internal combustion engines.

No licensing, legislative, regulatory or certification requirements apply to this unit at the time of publication.

Competency Field

Outdoor Power Equipment

Unit Sector

Technical

Elements and Performance Criteria

Elements Elements describe the essential outcomes.	Performance Criteria Performance criteria describe the performance needed to demonstrate achievement of the element. Where bold and italicised text is used, further information is detailed in the range of conditions section.
1. Prepare to service and repair post hole digging system	1.1 Job requirements are determined from workplace instructions 1.2 Service and repair procedures and information are sourced and interpreted 1.3 Hazards associated with the work are identified and risks are managed 1.4 Tools, equipment and materials are selected and checked for serviceability
2. Determine service and repair requirements of post hole digging system	2.1 System is inspected and tested according to manufacturer specifications, workplace procedures, and safety requirements 2.2 Faults are identified from inspection and causes of faults are determined 2.3 Inspection findings and test results are reported according to workplace procedures, and include recommendations for necessary service, repair or adjustment 2.4 Authorisation to proceed with service and repair is obtained according to workplace procedures
3. Carry out service and repair activities	3.1 Service and repair options are analysed and those most appropriate to the circumstances are selected 3.2 Tools, equipment and materials are selected and checked 3.3 Components are removed and inspected for serviceability according to manufacturer specifications, workplace procedures, and safety and environmental requirements 3.4 Reusable, repaired and replacement components are fitted and adjusted according to manufacturer specifications and workplace procedures
4. Check post hole digging system for normal operation	4.1 System is operated and compared to manufacturer specifications according to workplace procedures and safety requirements 4.2 Adjustments are made as required and post hole digging system is re-tested
5. Complete work processes	5.1 Final inspection is made to ensure work is to workplace expectations and equipment is presented ready for use, including protective guards, cowlings and safety features 5.2 Work area is cleaned, waste and non-recyclable material are disposed of and recyclable material is collected 5.3 Tools and equipment are checked and stored according to workplace procedures 5.4 Workplace documentation is processed according to workplace procedures

Foundation Skills

This section describes those language, literacy, numeracy and employment skills that are essential to performance and are not explicit in the performance criteria.

Skills	Description
Learning skills to:	locate appropriate sources of information efficiently.
Reading skills to:	interpret information from manufacturer and workshop literature when seeking post hole digging system specifications and procedures.
Writing skills to:	legibly and accurately fill out workplace documentation when reporting inspection findings, making repair recommendations, and recording parts and material used.
Numeracy skills to:	measure post hole digging system components and use basic mathematical operations, including addition and subtraction, to calculate distances, tolerances and deviations from manufacturer specifications.
Planning and organising skills to:	plan own work requirements and prioritise actions to achieve required outcomes and ensure tasks are completed within workplace timeframes.

Range of Conditions

This section specifies work environments and conditions that may affect performance. Essential operating conditions that may be present (depending on the work situation, needs of the candidate, accessibility of the item, and local industry and regional contexts) are included. Bold italicised wording, if used in the performance criteria, is detailed below.

Service and repair procedures must include:	inspecting, repairing and replacing components adjusting system and components lubricating gearbox testing repaired unit, including overload protection.
Safety requirements must include:	work health and safety (WHS) and occupational health and safety (OHS) requirements, including procedures for: safely starting and checking operation, adjustment and alignment of post hole digging system safely operating overload system selecting and using suitable personal protective equipment (PPE).
Environmental requirements must include:	procedures for trapping, storing and disposing of lubricating oils and greases released from post hole digging systems.

Unit Mapping Information

Equivalent to AURPTA2008 Service and repair post-hole digging systems

Links

Companion Volume implementation guides are found in VETNet2 - https://vetnet.education.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1