Assessment Requirements for AURTTA020 Apply heat induction processes

Release: 1

Assessment Requirements for AURTTA020 Apply heat induction processes

Modification History

Release	Comment
Release 1	New unit of competency.

Performance Evidence

Before competency can be determined, individuals must demonstrate they can perform the following according to the standards defined in this unit’s elements, performance criteria, range of conditions and foundation skills:

apply heat induction processes to three different chassis and component repairs, in which the work must involve the use of:

metal colours

heat crayons

thermal temp gun.

Knowledge Evidence

Individuals must be able to demonstrate knowledge of:

work health and safety (WHS) and occupational health and safety (OHS) requirements relating to applying heat induction processes, including procedures for:

selecting and using personal protective equipment (PPE)

using specialist heat induction equipment

identifying workplace hazards

environmental requirements, including procedures for trapping, storing and disposing of waste materials

heat induction process and procedures, including:

use of heat induction in repairs

use of heat induction equipment, including:

metal colours

heat crayons

thermal temp gun

original equipment manufacturer (OEM) or authorised agency specifications and recommended repair procedures

material types suitable for applying heat induction processes

problem-solving techniques relating to addressing repair defects

final inspection procedures

work area clean-up and maintenance requirements

procedures for completing workplace documentation.

Assessment Conditions

Assessors must satisfy NVR/AQTF assessor requirements.

Competency is to be assessed in the workplace or a simulated environment that accurately reflects performance in a real workplace setting.

Assessment must include direct observation of tasks.

Where assessment of competency includes third-party evidence, individuals must provide evidence that links them to having used heat induction equipment to repair vehicle chassis, e.g. repair orders.

Assessors must verify performance evidence through questioning on skills and knowledge to ensure correct interpretation and application.

The following resources must be made available:

automotive repair workplace or simulated workplace

workplace instructions

PPE required to use heat induction equipment

OEM or authorised agency repair procedures

heat induction equipment and operating instructions

three different damaged vehicle chassis and components requiring heat induction repairs

tools and equipment appropriate for applying heat induction processes.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=b4278d82-d487-4070-a8c4-78045ec695b1