Assessment Requirements for CPCCSG3004 Print digital signs

Release: 1

Assessment Requirements for CPCCSG3004 Print digital signs

Modification History

Release 1.

This version first released with CPC Construction, Plumbing and Services Training Package Version 2.

Revised unit of competency. Replaces superseded non-equivalent CPCCSI2004A Produce digital signage and CPCCSI3016A Produce digital signage using advanced software applications.

Performance Evidence

A person demonstrating competency in this unit must satisfy all of the elements, performance criteria and foundation skills of this unit, and must print three different signs from digital files on each of the following media:

aluminium composite

paper

vinyl.

At least one sign must be produced using a flatbed printer and one sign using a roll to roll digital printer.

Laminate one of the finished signs, selecting laminate for the printed substrate according to type of printed media and job requirements and safely and effectively undertaking laminating processes.

In doing the above work, the person must:

handle and use uncompressed file formats correctly in the digital printing process

apply digital colour management principles when using software and output media

correctly handle media used in the digital printing process

select and set up appropriate printers for the task and conduct routine maintenance appropriate to the printer

identify printing and laminating defects and rectify faults to ensure job requirements are met

operate raster image processor (RIP) software in the printing process.

Knowledge Evidence

A person demonstrating competency in this unit must demonstrate knowledge of:

characteristics of different types of digital printing output devices, including:

flatbed printers

roll to roll printers

ultraviolet (UV) printers

types and characteristics of various digital printing products

principles of colour theory and their application in printing digital signs

range and application of different laminates

techniques and process for laminating signs

safety data sheets (SDS) relevant to the use of printing tools and equipment

procedures for routine maintenance and cleaning of printers

statutory and regulatory authority requirements, particularly those relating to:

removal of waste products

storage of chemicals

terminology and use of abbreviations in the signs and graphics industry

use and application of uncompressed file formats, including:

encapsulated post script (EPS)

portable document format (PDF)

RAW file

tagged image file format (TIFF).

Assessment Conditions

Suitable assessment of performance requires:

equipment:

laminating equipment appropriate to the task

printing equipment appropriate to the task

materials:

electronic files prepared for printing

laminating film

printing media specified in performance evidence

specifications:

job requirements

manufacturer specifications

relationships with team members:

work may be conducted alone and in teams

timeframe:

according to job requirements.

Assessor requirements

As a minimum, assessors must satisfy the assessor requirements in the Standards for Registered Training Organisations (RTOs) current at the time of assessment.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=7e15fa6a-68b8-4097-b099-030a5569b1ad