Assessment Requirements for CPPSEC4019 Diagnose faults in networked security systems

Release: 1

Assessment Requirements for CPPSEC4019 Diagnose faults in networked security systems

Modification History

Release 1	This version first released with CPP Property Services Training Package Release 9.0. Supersedes and is equivalent to CPPSEC4019A Identify and diagnose security systems or network fault. Updated to meet the Standards for Training Packages.

Performance Evidence

To demonstrate competency, a candidate must meet the performance criteria of this unit by conducting testing and diagnostic procedures on three different networked security systems to diagnose:

a minimum of two system faults

a minimum of two network faults.

Knowledge Evidence

To be competent in this unit, a candidate must demonstrate knowledge of:

workplace policies and procedures that ensure compliance with legislative and regulatory requirements when diagnosing faults in networked security systems:

licensing requirements and limits of own authority

regulatory requirements in the jurisdiction of operation

requirements for complying with Australian Communications and Media Authority cabling rules

work health and safety

cable identification methods and techniques

common computer commands used to verify and manage internet protocol (IP) and network performance

difference between programming and configuration of security equipment and systems

documentation to be completed when diagnosing faults in networked security systems to ensure compliance with licensing and warranty requirements

fundamentals of routers, switches, firewalls and wireless access points

fundamentals of scripting language

keypad and control panel types and functions for a range of security equipment and systems

local area network and wide area network capabilities

meaning of multiple form factor authentication

methods for ensuring IP networked systems and equipment are properly secured

operational parameters and diagnostic testing procedures for a range of networked security systems:

access control systems

audible and visual warning devices

cameras and monitors

commercial and residential alarm systems

detection devices

electronic and mechanical fire safety and fire locking systems

electronic locks and locking systems

electronic readers

electronic screen equipment

intercoms and control panels

security doors and door controls

principles of security system networking and integration including IP addresses and devices

tests to confirm correct configurations, operation and connections for networked security systems

tools and equipment used when diagnosing faults in networked security systems

types of earthing systems used in electrical installations

typical hazards encountered when diagnosing faults in networked security systems and the control measures for each:

confined spaces

electrical

hazardous materials and chemicals

hidden utilities

people in the work area

power tools

vermin.

Assessment Conditions

Assessors must meet the requirements for assessors contained in the Standards for Registered Training Organisations.

All individuals engaged by a licensed RTO for security licensing purposes must hold both a security trainers licence (where such a licence exists within the relevant jurisdiction) and the licence for performing the security activities for which the individual is providing training or assessment. Regulators may impose other assessor conditions to meet jurisdictional assessment requirements.

Assessment must be conducted in the workplace or in a simulated workplace environment. Candidates must have access to:

legislation and licensing requirements that apply to diagnosing faults in networked security systems in the jurisdiction of operation

work instructions, specifications, documentation, networked security systems and tools required to achieve the performance evidence.

Links

Companion volumes to this training package are available at the VETNet website - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=7e15fa6a-68b8-4097-b099-030a5569b1ad