Assessment Requirements for FWPCOT3261 Transport forestry logs using trucks

Release: 1

Assessment Requirements for FWPCOT3261 Transport forestry logs using trucks

Modification History

Release	Comment
1	Replaces equivalent unit FPICOT3261 Transport forestry logs using trucks, which was first released with FPI11 Forest and Forest Products Training Package Version 2.2. This is the first release of this unit in the new standards format. Assessment requirements now specify the performance and knowledge evidence, as well as assessment conditions for this unit of competency. These sections simplify and replace components used in the previous unit format, including Required Skills and Knowledge, Evidence Guide and Range Statement

Performance Evidence

A person demonstrating competency in this unit must satisfy all of the elements, performance criteria and foundation skills of this unit. If a specific volume or frequency is not stated below, then evidence must be provided that the following requirements have been performed on at least one occasion:

plan the routes for and complete log movements using a truck or truck/trailer combination, in line with an individual work orders and transport schedule prescribing different load quantities, coupe locations and destinations for each job

assess the load during loading operations to avoid:

uneven weight distribution

instability or uncontrolled collapse of the load

assess the load during loading operations to account for:

requirements for trailer rigidity

turning clearance

overhang

projection above stanchions

crowning

weight distribution on truck and trailer axles

contact with bolsters, stanchions and other logs

after each of the above transportation movements, complete accurate basic records for log shifting processes and truck operating faults.

Knowledge Evidence

A person competent in this unit must be able to demonstrate knowledge of:

purpose and content of applicable commonwealth, state or territory transport regulations for driving heavy logging vehicles with particular emphasis on load limits, allowable dimensions, driving hours, fatigue management and required rest breaks

applicable fall from heights regulations and compliance requirements

environmental protection practices relevant to driving heavy logging trucks to minimise:

fuel consumption

emissions

noise

damage to soil, water and other aspects of habitat

key features of these varying environmental conditions and effects on driving heavy logging trucks:

sealed and unsealed roads and tracks

ground slope

ground hazards and obstacles

wind and dust

fog and rain

typical safety hazards present at loading and unloading facilities and methods used to minimise associated risks

methods used to:

plan time efficient routes and schedules to comply with regulations and environmental considerations

safely load, restrain and unload logs

features, capabilities and capacities of logging trucks and trailers

purpose, features and safe operation of equipment used to load, unload and transport logs:

log positioning equipment

load securing devices

overhang warning devices

communication equipment

organisational procedures specific to transporting, loading and unloading logs:

workplace health and safety with particular emphasis on rest breaks and use of personal protective equipment

communication reporting lines

recording and reporting log shifting processes and truck operating faults.

Assessment Conditions

The following resources must be made available:

logging trucks and trailers including one or more of the following:

rigid or articulated log trucks

semi-trailers

jinkers

quad-dogs

B doubles

two-bay skeletal trucks

safety fittings

head boards

cab guards

log positioning equipment including one or more of the following:

bolsters

slippers

stanchions

chocks

load securing devices including one or more of the following:

dogs and chains

binders/straps

webbing

lashings and winches

auto-tensioning devices

overhang warning devices including one or more of the following:

flags

lights

reflectors

signs

communication equipment including one or more of the following:

two-way radio

hands-free mobile phones

personal protective equipment suitable for loading and unloading trucks

maps for coupe location

work order and transport schedules with instructions for equipment allocation, transport requirements and location of coupe and destination for logs

template documents for recording log shifting processes and truck operating faults

organisational procedures for transporting, loading and unloading logs.

Competency is to be assessed in the workplace or a simulated environment that accurately reflects performance in a real workplace setting.

Assessor requirements

Assessors must:

hold the appropriate assessor competency standards as outlined in regulations; and

be able to demonstrate vocational competencies at least to the level being assessed; and

be able to demonstrate how they are continuing to develop their VET knowledge and skills as well as maintaining their industry currency and assessor competence.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=0d96fe23-5747-4c01-9d6f-3509ff8d3d47