Assessment Requirements for MEA231 Inspect, test and troubleshoot rotary wing aircraft automatic flight control systems and components

Release: 2

Assessment Requirements for MEA231 Inspect, test and troubleshoot rotary wing aircraft automatic flight control systems and components

Modification History

Release 2. Equivalent to MEA231 Inspect, test and troubleshoot rotary wing aircraft automatic flight control systems and components with amended prerequisite codes.

Performance Evidence

Evidence required to demonstrate competency in this unit must be relevant to and satisfy all of the requirements of the elements and performance criteria under the specified conditions of assessment, and must include:

applying relevant WHS practices

using approved maintenance documentation and aircraft publications relating to the automatic flight control and data system being maintained

recognition of system and component defects/external damage, correct installation, connection of plugs, terminations, and attaching hardware (including cabling/harnesses) and security in:

flight director components and interface

flight control components and interface

flight data recorders and interface

applying logic processes, taking and interpreting system measurements, using test equipment and appropriate wiring diagrams and manuals to accurately and effectively isolate malfunctions in the above systems

testing systems to isolate system malfunctions and assess post-maintenance serviceability.

It is essential that system testing procedures, cleanliness requirements and safety precautions applicable to the automatic flight control system being maintained are fully observed, understood and complied with. Ability to interpret inspection procedures and specifications (allowable limits) and apply them in practice across a range of inspection, testing and troubleshooting applications (including the timely involvement of supervisors or other trades) is critical.

Evidence of transferability of skills and knowledge related to inspection, testing and troubleshooting is essential. This is to be demonstrated through application across a range of rotary wing automatic flight control systems and components listed in the Assessment Conditions.

Knowledge Evidence

Evidence required to demonstrate competency in this unit must be relevant to and satisfy all of the requirements of the elements and performance criteria under the specified conditions of assessment, and include:

component attachment methods

explaining the basic layout (block diagram level), function and operation of:

flight director components and interface

flight control components and interface

flight data recorders and interface

explaining basic principles/functions relating to the above systems and associated with:

basic AC and DC circuit theory

digital fundamentals

analogue fundamentals

rotary wing flight theory

inner and outer loop control

rotary wing flight control system (mechanical, hydraulic and electro-mechanical types, trim and stabilisation)

flight control modes/channels

WHS requirements

system and component maintenance requirements and troubleshooting procedures

relevant maintenance manuals.

Assessment Conditions

Competency should be assessed in the workplace or simulated workplace using tools and equipment specified in the maintenance manuals. It is also expected that general and special purpose tools, and test and ground support equipment would be used where appropriate.

The application of testing procedures should clearly indicate knowledge of system operation, the relationship of individual components and the links with other systems (if applicable) within the limits of the aircraft/system fault-finding guide before undertaking any action. The work plan should take account of applicable safety and quality requirements in accordance with the industry and regulatory standards.

The following conditions of assessment represent the requirements of the Regulators (ADF and CASA) and maintenance stakeholders and must be rigorously observed.

A person cannot be assessed as competent until it can be demonstrated to the satisfaction of the workplace assessor that the relevant elements and performance criteria of the unit of competency are being achieved under routine supervision on at least one (1) item from each of the following groups:

flight director –indicators, computers, control boxes and interfaces with other systems

flight controls –servo actuators (roll, pitch, yaw and trim) computers and sensors

autopilot system –computers, sensors (gyros and/or accelerometers), controllers, mode selectors and system interface, CWS, disconnect, go around and trim switches.

This shall be established via the records in the Log of Industrial Experience and Achievement or, where appropriate, an equivalent Industry Evidence Guide (for details refer to the Companion Volume Assessment Guidelines).

Assessors must satisfy the requirements of the National Vocational Education and Training Regulator (Australian Skills Quality Authority, or its successors).

Where the unit is to be used for CASA licensing purposes the Assessor must also meet the criteria specified in the CASR Part 147 Manual of Standards.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=ce216c9c-04d5-4b3b-9bcf-4e81d0950371