Assessment Requirements for MSFFL3073 Mix and apply thin-film broadcast resin flooring systems

Release: 1

Assessment Requirements for MSFFL3073 Mix and apply thin-film broadcast resin flooring systems

Modification History

Release 1. New unit.

Performance Evidence

There must be evidence the candidate has completed the tasks outlined in the elements and performance criteria of this unit, and:

applied the following range of thin-film broadcast flooring systems in accordance with job requirements:

1 flake flooring system to an area of at least 10m2

1 flake flooring system to an area of more than 10m2

1 non-slip flooring system to an area of more than 10m2

1 broadcast flooring system (flake or non-slip) to an area of more than 50m2.

Knowledge Evidence

There must be evidence the candidate has knowledge of:

key aspects of state or territory legislation, regulations, standards and codes of practice, including individual technician rights and obligations relating to:

workplace health and safety

consumer law

environmental protection and sustainable use of materials

how to access supplier application notes

types, characteristics, uses and limitations of broadcast flooring systems

mathematical procedures for estimation and measurement, including calculation of area and use of ratios for mixing

types, uses and limitations of tools and equipment used in broadcast applications

characteristics and requirements of suitable substrate preparation, including different methods and products used to profile, repair, prime and clean

the features and layout of an effective mixing area

taping techniques to protect surfaces that aren’t to be coated, including walls, edges, transitions and boundaries on the floor

personal protective equipment (PPE) and correct usage

techniques for the following, the types of problems that may occur and how to avoid and respond:

measuring out and mixing broadcast flooring systems, including aggregate, pigment, fillers and stir-in additives

applying thin-film broadcast flooring systems, including broadcasting, cutting in, brushing, spreading with a squeegee and rolling

characteristics and requirements of suitable preparation between coats

quality indicators for finished flooring system

cleaning and storage procedures for PPE, tools, equipment and unused materials

disposal procedures for waste materials

requirements and protocols for recording, reporting and maintaining workplace records and information.

Assessment Conditions

The following aspects of the Performance Evidence must have been demonstrated and directly observed by the assessor in the workplace or in a simulated environment that reflects workplace conditions and contingencies:

application of a flake flooring system to an area of at least 10m2.

Remaining aspects of the Performance Evidence may be demonstrated in the workplace or in a simulated environment that reflects workplace conditions and contingencies but there is no requirement for direct observation by the assessor.

The following conditions must be met for this unit:

use of suitable facilities, equipment and resources, including:

locations requiring broadcast flooring

work orders

tools and equipment to complete tasks in the Performance Evidence, including safety and personal protective equipment

workplace procedures.

Assessors must satisfy the NVR/AQTF mandatory competency requirements for assessors.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=0601ab95-583a-4e93-b2d4-cfb27b03ed73