Assessment Requirements for MSFFM3026 Produce angled and curved components using manufactured board

Release: 1

Assessment Requirements for MSFFM3026 Produce angled and curved components using manufactured board

Modification History

Release 1. Changes to code, application, elements, performance criteria, assessment requirements. Foundation skills added. Range of conditions removed. Assessment requirements changed.

Performance Evidence

There must be evidence the candidate has completed the tasks outlined in the elements and performance criteria of this unit, and demonstrated the ability to:

produce at least 4 curved components using manufactured board, collectively including:

one kerfing method

one machine curved method

one laminated curve method

skinning a curved sub-frame

produce at least 2 angled components using manufactured board, collectively including:

one bevel join

one flat panel angled component.

Knowledge Evidence

There must be evidence the candidate has knowledge of:

workplace procedures for:

work health and safety

quality assurance

reporting of machinery faults and material defects

workflow for the construction process

how to:

interpret design documentation

prepare drawings and set-outs

techniques for producing curved and angled components using manufactured board, including machine and laminated curve methods and bevel joins

techniques for skinning a curved sub-frame

techniques for producing flat panel angled components

types and characteristics of manufactured board used for angled and curved components

tools and machinery used to create angle and curved components using manufactured board, including those used for bending and forming

personal protective equipment (PPE) required when creating angle and curved components using manufactured board

types and characteristics of adhesives used in cabinetry and furniture construction.

Assessment Conditions

Skills must have been demonstrated in the workplace or in a simulated environment that reflects workplace conditions and contingencies. The following conditions must be met for this unit:

use of suitable facilities, equipment and resources, including:

design documentation

unprocessed materials for construction

tools, equipment and machinery required for performance evidence

PPE

workplace procedures.

Assessors must satisfy the NVR/AQTF mandatory competency requirements for assessors.

Links

Companion Volume implementation guides are found in VETNet – - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=0601ab95-583a-4e93-b2d4-cfb27b03ed73