Assessment Requirements for MSFFM3044 Set up, operate and maintain computer numerically controlled (CNC) sizing machines

Release: 1

Assessment Requirements for MSFFM3044 Set up, operate and maintain computer numerically controlled (CNC) sizing machines

Modification History

Release 1. Changes to code, application, elements, performance criteria, assessment requirements. Foundation skills added. Range of conditions removed. Assessment requirements changed.

Performance Evidence

There must be evidence the candidate has completed the tasks outlined in the elements and performance criteria of this unit, and demonstrated the ability to:

set up, operate and complete operator maintenance on CNC sizing equipment to produce at least 3 different cutting patterns.

Knowledge Evidence

There must be evidence the candidate has knowledge of:

workplace procedure for:

quality assurance and tolerance levels

reporting of machinery faults and material defects

uses of CNC sizing machines:

CNC beam saws

double end profiling machines

CNC practices and techniques, including workflow process

characteristics of materials to be sized:

solid timber

manufactured board

laminate

solid synthetic materials and plastics.

Assessment Conditions

Skills must have been demonstrated in the workplace or in a simulated environment that reflects workplace conditions and contingencies. The following conditions must be met for this unit:

use of suitable facilities, equipment and resources required for performance evidence, including:

work documentation

unprocessed materials for cutting

CNC sizing machine

workplace procedures.

Assessors must satisfy the NVR/AQTF mandatory competency requirements for assessors.

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=0601ab95-583a-4e93-b2d4-cfb27b03ed73