PUADEFEO503C Conduct explosive ordnance packaging inspection

Revision Number: 1

PUADEFEO503C Conduct explosive ordnance packaging inspection

Modification History

Not applicable.

Unit Descriptor

Unit Descriptor	This unit covers the competency required to conduct an inspection of explosive ordnance packaging and to process the packaging for further action that may be required.

Application of the Unit

Application of the Unit	This competency normally applies to the individual who is required to conduct an inspection of explosive ordnance packaging and to process the packaging for further action that may be required. The inspection of the packaging is carried out in a logical sequence while adhering to all relevant occupational health and safety (OH&S) requirements. Processing the packaging is subject to the outcomes of the inspection and may result in damaged or defective packaging being rejected, disposed of, returned to the manufacturer or sent for maintenance.

Licensing/Regulatory Information

Not applicable.

Pre-Requisites

Pre-requisite Unit/s	Nil

Employability Skills Information

Employability Skills	This unit contains employability skills.

Elements and Performance Criteria Pre-Content

Elements describe the essential outcomes of a Unit of Competency.	Performance Criteria describe the required performance needed to demonstrate achievement of the element. Where bold italicised text is used, further information is detailed in the Required Skills and Knowledge and/or the Range Statement. Assessment of performance is to be consistent with the Evidence Guide.

Elements and Performance Criteria

ELEMENT	PERFORMANCE CRITERIA
1. Prepare for Inspection	1.1 Requirement for explosive ordnance packaging inspection is identified from work requests/instructions and is confirmed 1.2 OH&S requirements, including those contained in organisational procedures, are applied throughout the operation 1.3 Technical references, tools and equipment required for the inspection are identified, acquired and prepared in accordance with organisation procedures 1.4 Packaging is acquired, identified and accounted for, and moved or pre-positioned in preparation for inspection
2. Inspect explosive ordnance	2.1 Packaging is inspected in a logical set sequence to ensure that defects or damage are not overlooked in accordance with organisation policy and procedures, and technical specifications 2.2 Damage or other defects are identified and recorded in accordance with organisation procedures
3. Carry out post inspection procedures	3.1 Packaging is processed in accordance with organisation procedures 3.2 Documentation and records are maintained in accordance with statutory, organisation and workshop requirements

Required Skills and Knowledge

REQUIRED SKILLS AND KNOWLEDGE
This describes the essential skills and knowledge and their level, required for this unit.
Required Skills
apply OH&S requirements communicate orally and in writing identify faults, markings and labels maintain documentation process explosive ordnance packaging read, access, interpret and apply technical instructions and drawings related to packaging inspections
Required Knowledge
characteristics and limitations of packaging to be inspected inspection procedures organisational documentation requirements organisationalOH&S requirements

Evidence Guide

EVIDENCE GUIDE
Critical aspects for assessment and evidence required to demonstrate competency in this unit	Assessment must confirm the ability to comply with: organisational safety requirements appropriate legislative and regulatory requirements. Assessment must also confirm the ability to work safely within a workshop environment and to: identify packaging identify labelling and marking process explosive ordnance packaging maintain documentation. Consistency in performance Competency should be demonstrated in a range of actual or simulated reconditioning contexts.
Context of and specific resources for assessment	Context of assessment Competency should be assessed in the workplace or in a simulated work environment, in accordance with all relevant legislation and organisational requirements. Specific resources for assessment Access is required to: facilities and resources used in the reconditioning of explosive ordnance packaging.
Method of assessment	In a public safety environment assessment is usually conducted via direct observation in a training environment or in the workplace via subject matter supervision and/or mentoring, which is typically recorded in a competency workbook. Assessment is completed using appropriately qualified assessors who select the most appropriate method of assessment. Assessment may occur in an operational environment or in an industry-approved simulated work environment. Forms of assessment that are typically used include: direct observation interviewing the candidate journals and workplace documentation third party reports from supervisors written or oral questions.

Range Statement

RANGE STATEMENT
The Range Statement relates to the Unit of Competency as a whole. It allows for different work environments and situations that may affect performance. Bold italicised wording in the Performance Criteria is detailed below.
Packaging inspections may be conducted	As part of a work program On direction On receipt Prior to maintenance Prior to or post any activity
Organisation may include	Defence organisation Enterprises that work with explosive ordnance Other government departments or instrumentalities that work with explosive ordnance
Technical references may include	Technical drawings Technical reference pamphlets Orders and instructions Other publications
Packaging may be constructed from	Aluminium Bakelite Cardboard Fibreglass Plastic Polystyrene Rubber Steel Tin Wood
Inspections may include	Closing devices Desiccant indicators Handles Hinges Internal/external fitments Internal packaging Labels such as: free from explosives certification warning labels security seals special markings hazard labels contents labels un serial number shipping labels fraction label model/mark of packaging Pressure release valves Seals
Inspection may result in packaging being	Passed for use Recommended for sentencing Rejected
Explosive ordnance defects or damage may include	Corrosion Dents Fire damage Holes Non-compliance with technical specifications Tears
Processing may include	Disposal Rejection Retention for return or maintenance
Documentation and records may include	Receipt and issue records Timesheets Work records

Unit Sector(s)

Not applicable.