Assessment Requirements for RIIBHD305D Conduct down-hole hammer drilling

Release: 2

Assessment Requirements for RIIBHD305D Conduct down-hole hammer drilling

Modification History

Release	Comment
1	This unit replaces RIIBHD305 Conduct down-hole hammer drilling
2	Required frequency and volume of evidence amended in Performance evidence. Substantial amendments made in Assessment Conditions field, including: references to Industry Sectors, assessor and subject matter expert experience requirements, how assessment should be conducted and what it should confirm.

Performance Evidence

Evidence is required to be collected that demonstrates a candidate’s competency in this unit. Evidence must be relevant to the roles within this sector’s work operations and satisfy all of the requirements of the performance criteria of this unit and include evidence that the candidate:

locates and applies relevant legislation, documentation, policies and procedures

works effectively with others to undertake and complete conducting of down-hole hammer drilling that meets all of the required outcomes including:

uses a range of communication techniques and strategies to communicate and coordinate information and activity to other

communicates the hazards of cuttings in the return air stream to all crew members

demonstrates completion of conducting down-hole hammer drilling that safely, effectively and efficiently meets all of the required outcomes on more than one (1) occasion including:

correctly use the various rod/pipe handling equipment

correctly and competently add/remove rods/pipe from the string

correctly applies rotation speed and weight on the bit to maintain optimum performance

correctly measures line string components and calculate hole depth

correctly collars holes

ensure that samples are monitored for sample quality, correctly collected and handled

ensure that all string components are correctly maintained

disassembles, describes the function of components, inspect components, replace unserviceable parts and reassemble a DTH hammer

ensures that drill pipe is inspected regularly and wear rates monitored

ensure that threads are inspected and maintained

ensuring that bit sharpening equipment, used to sharpen TC bits are used correctly and safely and that bits are sharpened to correct tolerances

Knowledge Evidence

The candidate must demonstrate knowledge of conducting down-hole hammer drilling through:

the critical need to match like threads with like threads on all tubular components and make up torque requirements

the parameters relating to wear of drill pipe and integrity of threads

the function of hole collaring

the methods required to limit the contamination of samples

the theory behind TC bit sharpening

correct bit selection for different types of drilling and different ground conditions

identifying problems related to inaccurate measurement of bits and other related components

the importance of monitoring sample quantity

the role that blockages play in affecting sample quality

methods commonly used to clear down hole blockages in air drilled holes and the hazards associated with clearing blockages

methods used to clear a blockage in a sample delivery hose and the hazards associated with clearing blockages

the critical need for restraining devices to be fitted to all pressure delivery hoses and sample delivery hoses, the devices available and their methods of attachment

dangers of drilled samples being returned to the surface at high velocity in air drilling operations and the parameters involved

the importance of checking gauges and monitoring pressures, flow rates and temperatures

Assessment Conditions

An assessor of this unit must satisfy the requirements of the NVR/AQTF or their successors; and Industry regulations for certification and licensing: and,

this unit must be assessed in the context of this sector’s work environment; and,

this unit must be assessed in compliance with relevant legislation/regulation and using policies, procedures, processes and operational manuals directly related to the industry sector for which it is being assessed; and,

assessment may be conducted in conjunction with the assessment of other Units of Competency; and,

assessment must confirm consistent performance can be applied in a range of relevant workplace circumstances; and,

assessors must demonstrate the performance evidence, and knowledge evidence as outlined in this Unit of Competency, and through the minimum years of current* work experience specified below in an Industry sector relevant to the outcomes of the unit; or,

where the assessor does not meet experience requirements a co-assessment or partnership arrangement must exist between the qualified assessor and an Industry subject matter expert. The Industry subject matter expert should hold the unit being assessed (or an equivalent unit) and/or demonstrate equivalence of skills and knowledge at the unit level. An Industry technical expert must also demonstrate skills and knowledge from the minimum years of current work experience specified below in the Industry sector, including time spent in roles related to the unit being assessed; and,

assessor and Industry subject matter expert requirements differ depending on the Australian Qualifications Framework Level (AQF) of the qualification being assessed and/or Industry Sector as follows:

Industry sector	AQF** Level	Required assessor or Industry subject matter expert experience
Drilling, Metalliferous Mining, Coal Mining, Extractive (Quarrying) and Civil Construction	1	1 Year
2	2 Years
Drilling, Coal Mining and Extractive (Quarrying)	3-6	3 Years
Metalliferous Mining and Civil Construction	3-6	5 Years
Other sectors	Where this Unit is being assessed outside of the Resources and Infrastructure Sectors assessor and/or Industry subject matter expert experience should be in-line with industry standards for the sector in which it is being assessed and where no Industry standard is specified should comply with any relevant regulation.

*Assessors can demonstrate current work experience through employment within Industry in a role relevant to the outcomes of the Unit; or, for external assessors this can be demonstrated through exposure to Industry by conducting frequent site assessments across various locations.

**Where a unit is being delivered outside of a Qualification the first numeric character in the Unit code should be considered to indicate the AQF level

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=88a61002-9a21-4386-aaf8-69c76e675272