Assessment Requirements for RIIUND501D Implement the ventilation management plan

Release: 2

Assessment Requirements for RIIUND501D Implement the ventilation management plan

Modification History

Release	Comment
1	This unit replaces RIIUND501A Implement the ventilation management plan
2	Required frequency and volume of evidence amended in Performance evidence. Substantial amendments made in Assessment Conditions field, including: references to Industry Sectors, assessor and subject matter expert experience requirements, how assessment should be conducted and what it should confirm.

Performance Evidence

Evidence is required to be collected that demonstrates a candidate’s competency in this unit. Evidence must be relevant to the roles within this sector’s work operations and satisfy all of the requirements of the performance criteria of this unit and include evidence that the candidate:

locates and applies relevant legislation, documentation, policies and procedures

implements the requirements, procedures and techniques for the safe, effective and efficient implementation of the ventilation management plan including:

performing routine operational mathematical calculations (quantity, pressure, prediction)

interpreting and applying design criteria for ventilation systems and devices

interpreting computer spreadsheets and ventilation modelling/simulations

conducting enquiries/investigations and preparing reports

accessing, interpreting and applying data from monitoring systems and equipment

implementing the ventilation management training plan

applying risk management processes and techniques

implementing emergency response and evacuation procedures

demonstrates completion of the implementation of the ventilation management plan that safely, effectively and efficiently meets all of the required outcomes on more than one (1) occasion including:

operating hand held monitoring equipment

accessing and analysing ventilation information

measuring air quality and quantity

collecting, collating and interpreting ventilation data

auditing components of the ventilation management plan

Knowledge Evidence

The candidate must demonstrate knowledge in implementing the ventilation management plan through:

methods of mine ventilation and their applications/limitations including:

exhaust/force

antitropal

homotropal

flank returns

ascensional/descensional

bleeder

Z/U/Y systems

other combinations

methods of panel ventilation and their applications/limitations including:

homotropal and antitropal auxiliary fans

coursed ventilation (narrow side/wide side)

machine mounted scrubber systems

compressed air venturis and bleeders

impact of mine and panel design on ventilation

mine roadways and shafts and their impact on mine ventilation

impact of material characteristics and seam gradients on mine ventilation design

impacts on ventilation system of gas drainage, spontaneous combustion, outburst and windblast

mine gases; types and characteristics, sources, physiological effects and methods of detection

dust, fumes and other particulate matter; the types, sources, physical and physiological effect and control/mitigation methods

mine fires; the types, sources of ignition, possible effects on the ventilation circuit and prevention/control/mitigation methods

mine explosions; types, ignition sources, possible effects on the ventilation circuits and prevention/control/mitigation methods

pressure changes; causes, impacts on the ventilation system, and responses (to include the causes and effects of natural ventilation and re-circulation)

heat/humidity; sources and factors which may impact on mine ventilation and personnel

mine fans including:

ventilation control devices; types, purposes, design criteria and specifications, distribution/placement criteria and limitations

de-gassing; methods of control – including brattice, auxiliary fans, compressed air venturis, sails, hurdles and bleeders

fixed ventilation monitoring systems types, uses and limitations

basic computer-based systems used for mine ventilation monitoring and analysis

ventilation surveys; the types, frequency and method for conducting

ventilation theory including:

psychrometry and heat

gas laws including Charles and Boyle

natural ventilation pressures

air quality measurement

control device leakage

duct leakage

regulator

equivalent office calculation and Kirchoff’s laws

Assessment Conditions

An assessor of this unit must satisfy the requirements of the NVR/AQTF or their successors; and Industry regulations for certification and licensing; and,

this unit is best assessed in the context of this sector’s work environment;

where personal safety or environmental damage are limiting factors, assessment may occur in a simulated environment provided it is realistic and sufficiently rigorous to cover all aspects of this sector’s workplace performance, including environment, task skills, task management skills, contingency management skills and job role environment skills; and,

this unit must be assessed in compliance with relevant legislation/regulation and using policies, procedures, processes and operational manuals directly related to the industry sector for which it is being assessed; and,

assessment may be conducted in conjunction with the assessment of other Units of Competency; and,

assessment must confirm consistent performance can be applied in a range of relevant workplace circumstances; and,

assessors must demonstrate the performance evidence, and knowledge evidence as outlined in this Unit of Competency, and through the minimum years of current* work experience specified below in an Industry sector relevant to the outcomes of the unit; or,

where the assessor does not meet experience requirements a co-assessment or partnership arrangement must exist between the qualified assessor and an Industry subject matter expert. The Industry subject matter expert should hold the unit being assessed (or an equivalent unit) and/or demonstrate equivalence of skills and knowledge at the unit level. An Industry technical expert must also demonstrate skills and knowledge from the minimum years of current work experience specified below in the Industry sector, including time spent in roles related to the unit being assessed; and,

assessor and Industry subject matter expert requirements differ depending on the Australian Qualifications Framework Level (AQF) of the qualification being assessed and/or Industry Sector as follows:

Industry sector	AQF** Level	Required assessor or Industry subject matter expert experience
Drilling, Metalliferous Mining, Coal Mining, Extractive (Quarrying) and Civil Construction	1	1 Year
2	2 Years
Drilling, Coal Mining and Extractive (Quarrying)	3-6	3 Years
Metalliferous Mining and Civil Construction	3-6	5 Years
Other sectors	Where this Unit is being assessed outside of the Resources and Infrastructure Sectors assessor and/or Industry subject matter expert experience should be in-line with industry standards for the sector in which it is being assessed and where no Industry standard is specified should comply with any relevant regulation.

*Assessors can demonstrate current work experience through employment within Industry in a role relevant to the outcomes of the Unit; or, for external assessors this can be demonstrated through exposure to Industry by conducting frequent site assessments across various locations.

**Where a unit is being delivered outside of a Qualification the first numeric character in the Unit code should be considered to indicate the AQF level

Links

Companion Volume implementation guides are found in VETNet - https://vetnet.gov.au/Pages/TrainingDocs.aspx?q=88a61002-9a21-4386-aaf8-69c76e675272