TLIC3031A Stable a heritage steam locomotive

Release: 1

TLIC3031A Stable a heritage steam locomotive

Modification History

Not Applicable

Unit Descriptor

Unit Descriptor	This unit involves the skills and knowledge required to stable a heritage steam locomotive in accordance with relevant workplace practices, rail regulations and codes of practice. It includes determining the required stabling location, shunting and securing the train, stabling and securing the heritage steam locomotive, carrying out all required post-operational checks and completing post-operational paperwork. This unit replaces part of the previous unit TDTC1401A Prepare, operate, monitor and stable heritage steam locomotive. Licensing, legislative, regulatory or certification requirements are applicable to this unit.

Application of the Unit

Application of the Unit	Persons achieving competence in this unit will need to fulfil the applicable legislated rail safety requirements including acts and regulations from each state and territory together with any nationally approved compliance codes and/or guidelines and local rail regulations and codes of practice as they apply to the operation of heritage railway systems. Work is performed under minimal supervision, generally within a team environment. It involves the application of routine operational principles and procedures to the stabling and securing a steam locomotive across a variety of operational contexts in the Australian heritage rail system.

Licensing/Regulatory Information

Refer to Unit Descriptor

Pre-Requisites

Not Applicable

Employability Skills Information

Employability Skills	This unit contains employability skills.

Elements and Performance Criteria Pre-Content

Elements describe the essential outcomes of a unit of competency.	Performance criteria describe the required performance needed to demonstrate achievement of the element. Assessment of performance is to be consistent with the evidence guide.

Elements and Performance Criteria

ELEMENT	PERFORMANCE CRITERIA
1 Determine stabling location	1.1 Contact is made with train controller and yard staff to determine planned location for stabling the steam locomotive 1.2 Directions of train controller and yard staff are interpreted and followed 1.3 Care is taken to keep clear of other roads
2 Stable and shut down steam locomotive	2.1 Carriages or vehicles are shunted and secured in accordance with directions, workplace procedures and rail regulations 2.2 Steam locomotive is stabled in correct location as directed 2.3 Derailers are set in place as per workplace procedures and rail regulations 2.4 Handbrakes are applied 2.5 Park brakes are secured 2.6 Steam locomotive is stabled as per operator's instructions and workplace procedures 2.7 Cab is secured as per workplace procedures
3 Carry out post-operational checks	3.1 Fluid and fuel levels are checked and any required action is taken to top up levels 3.2 Visual check is made of steam locomotive as per workplace procedures 3.3 Any identified faults and defects are fixed or reported and recorded as per workplace procedures 3.4 Faulty and defective equipment that presents a safety risk is isolated and tagged as per workplace procedures and rail regulations 3.5 Outcomes of post-operational checks are recorded as per workplace procedures
4 Complete post-operational paperwork	4.1 Timesheet or other work record is completed 4.2 Roster is checked for future work allocation 4.3 Issues and variations are discussed and resolved with roster clerk 4.4 All required safeworking documentation and actions are completed as per workplace procedures and rail regulations 4.5 All equipment is returned and stowed as per workplace requirements

Required Skills and Knowledge

REQUIRED KNOWLEDGE AND SKILLS
This describes the essential knowledge and skills and their level required for this unit.
Required knowledge:
Applicable legislated rail safety requirements including acts and regulations from each state and territory together with any nationally approved compliance codes and/or guidelines and local rail regulations and codes of practice as they relate to heritage railway operations
Relevant OH&S and environmental procedures and regulations
Steam locomotive controls, instruments and indicators and their purpose, location and use
Procedures for operating and stabling a steam locomotive
Braking and safety system procedures
Operating controls to start, accelerate, decelerate and stop a steam locomotive
Speed and load limits
Procedures for managing hazardous situations when operating and stabling a steam locomotive
Procedures for operating and shutting down ancillary systems
Procedure for completing relevant documentation when stabling a steam locomotive
Procedures to be followed in the event of an emergency
Procedures for minor maintenance, cleaning, lubricating and servicing of steam locomotives
Procedures for identifying equipment defects, assessing and reporting for appropriate action
Monitoring devices; braking and power equipment, auxiliary systems, and signalling systems
Local procedures and operating requirements
Typical defects that can occur on a steam locomotive and related action that should be taken
Procedures for operating electronic communications equipment with required protocol

Required skills:
Communicate effectively with others when stabling a heritage steam locomotive
Read and interpret instructions, procedures and information relevant to the stabling of a steam locomotive
Interpret and follow operational instructions and prioritise work
Complete documentation related to the stabling of a steam locomotive
Operate electronic communications equipment to required protocol
Work collaboratively with others when stabling a steam locomotive
Identify and assess steam locomotive defects and deficiencies and take appropriate action to report, isolate, repair or replace any identified defective equipment as per workplace procedures
Satisfactorily manage unplanned events
Apply precautions and required action to minimise, control or eliminate hazards that may exist when stabling a steam locomotive
Recognise problems that may arise when stabling a steam locomotive and take appropriate action
Check and replenish fluids and fuel and carry out lubrication requirements on a steam locomotive
Modify activities depending on differing operational contingencies, risk situations and environments
Adapt to differences in steam locomotives and associated equipment and procedures
Select and use required personal protective equipment conforming to industry and OH&S standards
Conduct an inspection of a steam locomotive
Document outcomes of inspection of a steam locomotive
Stable a steam locomotive after service

Evidence Guide

EVIDENCE GUIDE
The evidence guide provides advice on assessment and must be read in conjunction with the performance criteria, required knowledge and skills, the range statement and the assessment guidelines for this Training Package.
Critical aspects for assessment and evidence required to demonstrate competency in this unit	The evidence required to demonstrate competency in this unit must be relevant to and satisfy all of the requirements of the elements and performance criteria of this unit and include demonstration of applying: the underpinning knowledge and skills relevant legislation and workplace procedures other relevant aspects of the range statement
Context of and specific resources for assessment	Performance is demonstrated consistently over a period of time and in a suitable range of contexts Resources for assessment include: a range of relevant exercises, case studies and/or other simulated practical and knowledge assessment, and/or access to an appropriate range of relevant operational situations in the workplace In both real and simulated environments, access is required to: relevant and appropriate materials and equipment, and applicable documentation including workplace procedures, regulations, codes of practice and operation manuals
Method of assessment	Assessment of this unit must be undertaken by a registered training organisation As a minimum, assessment of knowledge must be conducted through appropriate written/oral tests Practical assessment must occur: through activities in an appropriately simulated environment at the registered training organisation, and/or in an appropriate range of situations in the workplace

Range Statement

RANGE STATEMENT
The range statement relates to the unit of competency as a whole. It allows for different work environments and situations that may affect performance.
Operations may be conducted:	by day or night in all relevant weather conditions
Heritage steam locomotives may include:	any heritage steam locomotives in service within Australia
Equipment on a steam locomotive may include:	steam locomotive instrumentation (gauges) feed water controls boiler controls and safety devices braking systems driving and other operational controls communication systems warning equipment ancillary systems vigilance systems traction systems head and marker lights
Inspection of a heritage steam locomotive may include:	lights and power systems hoses couplings head boards doors and door locks suspension brake equipment wheels seals sand and fuel boiler and mountings cables glass windows and doors audible faults (e.g. hiss of escaping air or steam) visible faults (e.g. oil leaks, tears and cracks)
Communications equipment may include:	portable and fixed two way radio mobile phone
Auxiliary equipment may include:	steam regulator cab sprinkler gauges generator sandboxes whistle steam turbine generator all ancillary valves hand brake injectors lubricators gauge glasses blower damper cylinder cocks mechanical stoker oil burning apparatus
Post operation checks may include:	lubrication system checking for fluid leaks brake testing checking of fluid and fuel levels
Risk minimisation may require differentiating between faults, defects and deficiencies that:	do not present a hazard and could be attended to under running maintenance or in a normal maintenance schedule present a potential hazard and need to be attended to under running maintenance or at the next most practical opportunity present an immediate hazard and require immediate attention
Relevant personnel may include:	train crew train controllers and signallers rostering supervisors and staff other train drivers and crews depot coordinators yard masters, supervisors and other operational personnel service delivery supervisors station yard staff maintenance personnel immediate internal or external customers
Action taken upon the identification of faults, defects or deficiencies may include:	reporting the problem and carrying out repairs (depending on the level and extent of work required), or isolating and tagging the faulty equipment and advising appropriate personnel of the fault and need for repair or replacement
Depending on the organisation concerned workplace procedures may be called:	standard operating procedures company procedures enterprise procedures organisational procedures established procedures
Safety and personal protective equipment may include:	gloves sunscreen and sunglasses safety glasses insect repellent safety headwear and footwear two-way radios hand lamps flags safety devices audible indicators breathing equipment fire extinguishers high visibility clothing hearing protection
Positioning of heritage motive power unit may involve:	operation of manual points operation of turntable coupling/uncoupling to other rolling stock
Information and documents may include:	applicable legislated rail safety requirements including acts and regulations from each state and territory together with any nationally approved compliance codes and/or guidelines steam locomotive operational records and user log books maintenance notices, records and requests preparation sheets certificates and service dockets train running sheets time sheets roadworthy certificate train wire (status list, dangerous goods list, consist information, etc.) operational instructions, policies and procedures, including: those related to preventing steam locomotives from moving; track speed, length and load limitations; monitoring and complying with signals; and procedures for operating in accordance with specific track conditions emergency procedures manual
Applicable legislation, regulations and codes may include:	applicable legislated rail safety requirements including acts and regulations from each state and territory together with any nationally approved compliance codes and/or guidelines relevant Australian Standards and related requirements relevant state/territory OH&S legislation relevant state/territory environmental protection legislation

Unit Sector(s)

Not Applicable

Competency Field

Competency Field	C - Vehicle Operation