TLIC3087A Operate a rear loading mobile compaction/collection vehicle

Release 1

TLIC3087A Operate a rear loading mobile compaction/collection vehicle

Modification History

Release 1. This is the first release of this unit.

Unit Descriptor

This unit involves the skills and knowledge required to operate a rear loading mobile compaction/collection vehicle (the ‘vehicle’).

Licensing, legislative, regulatory and certification requirements are applicable to this unit.

Application of the Unit

Vehicle must be operated in compliance with vehicle licence requirements and regulations relating to the relevant state/territory and traffic authorities.

Vehicle is operated with limited or no supervision, with accountability and responsibility for self and others in achieving the prescribed outcomes.

Licensing/Regulatory Information

Refer to Unit Descriptor.

Pre-Requisites

Nil

Employability Skills Information

This unit contains employability skills.

Elements and Performance Criteria Pre-Content

Elements describe the essential outcomes of a unit of competency.	Performance criteria describe the required performance needed to demonstrate achievement of the element. Assessment of performance is to be consistent with the evidence guide.

Elements and Performance Criteria

1	Follow safety requirements	1.1	Operator and third party safety is observed in accordance with organisational/manufacturer and legislative requirements
1.2	Vehicle controls are checked and operated in accordance with organisational/manufacturer requirements
1.3	Vehicle cleaning and non-technical maintenance is undertaken in accordance with organisational/manufacturer requirements
1.4	Safety items are used and stored in accordance with organisational/manufacturer requirements
1.5	Defective equipment is reported in accordance with organisational/manufacturer requirements
2	Load product onto vehicle	2.1	Vehicle is made ready to operate in accordance with organisational/manufacturer requirements
2.2	Product streams to be collected are identified
2.3	Documentation provided is used to determine locations to collect product
2.4	Product is deposited into vehicle collection area (hopper) in accordance with organisational/manufacturer and legislative requirements
2.5	Blockages and non-compliant product are cleared in accordance with organisational/manufacturer and legislative requirements
2.6	Prior to travel, product is removed from ground and no product is left on lifting equipment, vehicle or body
3	Compact product in vehicle	3.1	Loading of product within the body of the vehicle is monitored
3.2	Compaction equipment is operated in accordance with organisational/manufacturer requirements
3.3	Once vehicle reaches gross vehicle mass (GVM) compaction/loading is ceased in accordance with relevant organisational/manufacturer and legislative requirements
4	Unload product from vehicle and complete relevant documentation	4.1	Vehicle is positioned on level, stable ground to ensure vehicle safety and stability when unloading
4.2	Vehicle is positioned to allow unloading, in accordance with site, organisational/manufacturer and legislative requirements
4.3	Unloading equipment is operated in accordance with organisational/manufacturer and legislative requirements
4.4	Return of equipment used to transit position is ensured
4.5	Documentation for unloaded product is completed in accordance with organisational/manufacturer and legislative requirements

Required Skills and Knowledge

This section describes the knowledge and skills required for this unit.
Required knowledge:
Efficient driving techniques and eco-driving considerations
Factors involved in trip preparation
Factors that may cause traffic delays and diversions
Relevant dangerous goods (DG) information relating to operating the vehicle
Relevant state and territory roads and traffic authority road rules, regulations, permits and licence requirements
Relevant work health and safety (WHS)/occupational health and safety (OHS) and environmental procedures and regulations relating to vehicle operations
Safe pickup and delivery of product to and from site
Vehicle loading and unloading procedures
Workplace documentation
Workplace driving and operational instructions

Required skills:
Adapt appropriately to cultural differences in the workplace and customer sites, including modes of behaviour and interaction with others
Apply fatigue management knowledge and techniques
Apply precautions and required action to minimise, control or eliminate hazards that may exist when operating the vehicle
Complete documentation relating to the vehicle
Implement contingency plans for unexpected events when operating the vehicle
Identify, load and transport product streams in accordance with organisational/manufacturer and legislative requirements
Interpret and follow operational instructions and prioritise work
Manually position product containers/bins
Modify activities depending on operational contingencies, risk situations and environments
Monitor and anticipate traffic hazards and take appropriate action
Monitor performance of vehicle and equipment and take appropriate action where required
Operate and adapt to differences in equipment in accordance with standard operating procedures
Read and interpret instructions, procedures, information and signs relevant to the vehicle
Select and use required personal protective equipment (PPE), conforming to organisational, industry and WHS/OHS standards
Work collaboratively with others when operating the vehicle
Work systematically with required attention to detail, without injury to self or others or damage to infrastructure or equipment

Evidence Guide

The evidence guide provides advice on assessment and must be read in conjunction with the performance criteria, required knowledge and skills, the range statement and the assessment guidelines for this Training Package.
Critical aspects for assessment and evidence required to demonstrate competency in this unit	The evidence required to demonstrate competence in this unit must be relevant to and satisfy all of the requirements of the Elements, Performance Criteria, Required Skills, Required Knowledge and include: applying techniques for loading and unloading vehicle applying correct operation of vehicle cabin functions using correct manual handling techniques when operating vehicle and/or product containers identifying and using the PPE required for the product being loaded/transported applying eco-driving techniques when operating the vehicle knowledge of relevant legislation, and organisational and manufacturer procedures for transporting product in the vehicle knowledge of customer requirements when picking up product or delivering product to a product collection facility.
Context of and specific resources for assessment	Performance is demonstrated consistently over time and in a suitable range of contexts. Resources for assessment include access to: relevant and appropriate materials and equipment to meet performance criteria applicable documentation, including workplace procedures, regulations, codes of practice and operating manuals.
Method of assessment	Practical assessment must: occur in three different aspects of the job function in the workplace ensure written and verbal understanding of all types of product to identify compatibility. A range of assessment methods should be used to assess practical skills and knowledge. Use of a simulator is not suitable for final assessment of this unit of competency.

Range Statement

The range statement relates to the unit of competency as a whole. It allows for different work environments and situations that may affect performance.
Equipment fitted to the vehicle may include:	emergency information holder emergency shutdown controls eyewash kit fire extinguishers first aid kit spill kit vehicle emergency equipment
Loading and unloading sites may include:	council sites customer site depot private sites waste, transfer or recycling sites
Personal safety measures may include:	conflict management techniques correct use of safety rails and walkways fitness for duty hearing protection high visibility clothing location of pinch points manual handling techniques PPE required for the product class being transported safety footwear three points of contact when accessing/egressing vehicle/body
Eco driving includes:	braking efficiently ensuring transmission control not over-revving engine observing speed limits using auxiliary braking controls vehicle sympathy
Factors that may cause traffic delays and diversions include:	bridge or tunnel damage building construction emergency situations such as bushfires, flooding, changes in weather holiday traffic inefficient run planning livestock movement road closures for utility works such as electricity, water, sewerage or telecommunications road damage/road works traffic accidents vehicle breakdowns
Workplace procedures may include:	established manufacturer organisational regulatory/codes of practice
Documentation and records may include:	daily driver run sheet environmental documents pertaining to state of operation fatigue documentation mass/work diary vehicle reporting documentation
Applicable procedures and codes may include:	Relevant state/territory procedures and codes for the vehicle including: fatigue management relations licensing rules mass management regulations permit requirements road and traffic rules WHS/OHS and environmental legislation

Unit Sector(s)

Not applicable.

Competency Field

C – Vehicle Operation