TLIS3025A Implement ballast unloading

Release: 1

TLIS3025A Implement ballast unloading

Modification History

Not Applicable

Unit Descriptor

Unit Descriptor	This unit involves the skills and knowledge required to implement ballast unloading in accordance with safeworking and regulatory requirements and workplace procedures. It includes determining the job requirements, carrying out the unloading activity in accordance with work orders, and completing all required documentation. Licensing or certification requirements may be applicable to this unit.

Application of the Unit

Application of the Unit	Persons achieving competence in this unit will need to fulfil the applicable legislated rail safety requirements including acts and regulations from each state and territory together with any nationally approved compliance codes and/or guidelines. Work is performed under limited supervision, generally within a team environment. It involves the application of routine operational principles and procedures to implement ballast unloading as part of workplace activities across a variety of operational context within the Australian rail system. Operators of mechanised equipment must have undertaken training and, where appropriate, hold the relevant licence, permit or certificate and be recognised as competent for the class of machinery being used.

Licensing/Regulatory Information

Refer to Unit Descriptor

Pre-Requisites

Not Applicable

Employability Skills Information

Employability Skills	This unit contains employability skills.

Elements and Performance Criteria Pre-Content

Elements describe the essential outcomes of a unit of competency.	Performance criteria describe the required performance needed to demonstrate achievement of the element. Assessment of performance is to be consistent with the evidence guide.

Elements and Performance Criteria

ELEMENT	PERFORMANCE CRITERIA
1 Determine job requirements	1.1 Work requirements are determined for new ballast work and/or repair of existing ballast 1.2 Obstacles in work area are identified and removal or protection are organised as necessary to ensure smooth workflow following workplace procedures 1.3 Resources are organised to meet the scope of the job and work methods selected 1.4 Ballast quantities are determined
2 Undertake ballast unloading	2.1 Appropriate site communications are established and agreed to ensure safe and efficient working conditions 2.2 Ballast unloading operation is implemented to ensure appropriate flow rates and extent 2.3 Ballast is distribution by manual and/or mechanical methods to allow safe operation of trains 2.4 Ballast is removed from sensitive infrastructure to ensure safe operation of trains and safety of public
3 Complete documentation	3.1 Documentation is completed in line with workplace requirements

Required Skills and Knowledge

REQUIRED KNOWLEDGE AND SKILLS
This describes the essential knowledge and skills and their level required for this unit.
Required knowledge:
Relevant safety, OH&S and environmental procedures and regulations
Workplace procedures for the implementation of ballast unloading activities
Problems that may occur when implementing track ballast activities, and action that can be taken to report or resolve the problems
Hazards that may exist when implementing track ballast activities, and ways of controlling the risks involved
Functions of ballast
Required standard of materials and methods involved in implementing ballast unloading activities
Ballast flow rates
Ballast hopper operation
Contents of workplace technical manuals relating to ballast unloading and profile
Relevant recording and documentation procedures

Required skills:
Agree on communication methods and communicate effectively with others including train drivers and equipment operators when implementing ballast unloading activities
Read and interpret technical plans, specifications, instructions and manuals relevant to implementing ballast unloading activities
Interpret and follow operational instructions and prioritise work when implementing ballast unloading activities
Complete documentation related to implementing ballast unloading activities
Operate communication equipment to required protocol
Work collaboratively with others when implementing ballast unloading activities
Promptly report and/or rectify any identified problems, faults or malfunctions that may occur when implementing ballast unloading activities in accordance with regulatory requirements and workplace procedures
Plan own and team work including predicting consequences and identifying improvements
Monitor work activities in terms of planned schedule
Modify activities depending on differing operational contingencies, risk situations and environments
Work systematically with required attention to detail without injury to self or others, or damage to equipment
Select and use required personal protective equipment
Select and use relevant equipment and tools

Evidence Guide

EVIDENCE GUIDE
The evidence guide provides advice on assessment and must be read in conjunction with the performance criteria, required knowledge and skills, the range statement and the assessment guidelines for this Training Package.
Critical aspects for assessment and evidence required to demonstrate competency in this unit	The evidence required to demonstrate competency in this unit must be relevant to and satisfy all of the requirements of the elements and performance criteria of this unit and include demonstration of applying: the underpinning knowledge and skills relevant legislation and workplace procedures other relevant aspects of the range statement Assessment must include exercises which demonstrate competent performance of the following in a range of situations: determining job requirements and ensuring unloading operation is carried out correctly ensuring ballast is distributed so as to meet requirements for safe operation completing documentation according to workplace requirements
Context of and specific resources for assessment	Performance is demonstrated consistently over a period of time and in a suitable range of contexts Resources for assessment include: a range of relevant exercises, case studies and/or other simulated practical and knowledge assessment, and/or access to an appropriate range of relevant operational situations in the workplace In both real and simulated environments, access is required to: relevant and appropriate materials and equipment, and applicable documentation including workplace procedures, regulations, codes of practice and operation manuals
Method of assessment	Assessment of this unit must be undertaken by a registered training organisation As a minimum, assessment of knowledge must be conducted through appropriate written/oral tests Practical assessment must occur: through activities in an appropriately simulated environment at the registered training organisation, and/or in an appropriate range of situations in the workplace

Range Statement

RANGE STATEMENT
The range statement relates to the unit of competency as a whole. It allows for different work environments and situations that may affect performance.
Operations may be conducted:	by day or night in all weather conditions
Work may be conducted in:	restricted spaces exposed conditions controlled or open environments
Work may involve:	exposure to chemicals, and dangerous or hazardous substances movements of equipment, goods and vehicles
Equipment may include:	front end loaders ballast hoppers road trucks hand tools and small plant ballast forks other mechanical means
Materials may include:	gravel ballast crushed rock ballast metal fines/road base
Obstructions may include:	underbridges turnouts signalling equipment train detection equipment level crossings lubrication equipment
Methods may include:	placing ballast with: ballast hoppers off-track plant ballast regulators ballast cleaning equipment distributing ballast with: ballast ploughs ballast cleaning equipment off-track plant ballast regulators manual methods
Communications equipment may include:	two-way radios telephones/mobile phones
Depending on work context, safety and personal protective equipment may include:	high visibility clothing hearing protection gloves sunscreen sunglasses dust mask safety glasses insect repellent safety headwear safety footwear portable radios/radio headsets or mobile phone hand lamps flags safety devices
Depending on the type of organisation concerned and the local terminology used, workplace procedures may include:	company procedures enterprise procedures organisational procedures established procedures
Information/documents may include:	operational instructions, policies and workplace procedures local authority regulations and procedures work orders technical instructions manufacturers or workplace equipment instructions and operation manuals emergency procedure manuals two-way radio/mobile phone operation procedures QA plans, data and document control conditions of service, legislation and industrial agreements including workplace agreements and awards
Applicable procedures and codes may include:	legislated rail safety requirements including acts and regulations from each applicable state and territory together with any nationally approved compliance codes and/or guidelines relevant Australian Standards and related requirements, including AS 4292 relevant state/territory OH&S legislation relevant state/territory environmental protection legislation

Unit Sector(s)

Not Applicable

Competency Field

Competency Field	S - Construction and Installation